{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["ENERGIA","CONEXION","REP_MTTO","COR_RECONEX"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ENERGIA","index":0,"n_rows":150,"n_cols":30,"rows_kept":150,"cut":false,"hidden":false,"merged":[[1,0,1,1],[2,0,2,5],[147,7,147,12],[147,13,147,18]]}
["PLIEGO TARIFARIO DEL SERVICIO PUBLICO DE ELECTRICIDAD (NO INCLUYE IGV)"]
["2022-10-04",{"$nulls":14},"VIGENTE A PARTIR DEL DIA 04-10-2022"]
["SISTEMA ELECTRICO",{"$nulls":6},"Cusco","Valle Sagrado 1","Valle Sagrado 2","Valle Sagrado 3","Sicuani","Sicuani Rural","Combapata-Chumbivilcas","Yauri","La Convención Macupicchu","La Convención Rural","Abancay","Abancay Rural-Chuquibambilla-Chacapuente","Andahuyalas","Puerto Maldonado","Puerto Maldonad Rural, Iñapari, Iberia","Mazuko","SER-Apurimac y Valle Sagrado","SER-Valle Vilcanota","SER-Quispicanchis","SER-Espinar","SER-Iberia","SER-Machupicchu","SER-Mazuko"]
[]
["MEDIA TENSION",{"$nulls":5},"UNIDAD",{"$nulls":10},"TARIFA"]
["MT2","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",34.43,34.29,34.43,34.29,34.93,34.93,34.93,35.340000000000003,33.369999999999997,33.369999999999997,34.29,34.29,34.29,37.270000000000003,37.270000000000003,34.64,34.29,34.93,34.43,35.340000000000003,37.270000000000003,33.369999999999997,34.64]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",28.62,28.54,28.62,28.54,29.02,29.02,29.02,29.42,27.86,27.86,28.54,28.54,28.54,29,29,28.46,28.54,29.02,28.62,29.42,29,27.86,28.46]
[null,"Cargo por Potencia Activa de Generación en HP",{"$nulls":4},"S/./kW-mes",71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995,71.489999999999995]
[null,"Cargo por Potencia Activa por uso de redes de Distribución en HP",{"$nulls":4},"S/./kW-mes",22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92,22.92]
[null,"Cargo por Exceso de Potencia Activa por uso de redes de Distribución en HFP",{"$nulls":4},"S/./kW-mes",23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46,23.46]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19]
["MT3","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",34.43,34.29,34.43,34.29,34.93,34.93,34.93,35.340000000000003,33.369999999999997,33.369999999999997,34.29,34.29,34.29,37.270000000000003,37.270000000000003,34.64,34.29,34.93,34.43,35.340000000000003,37.270000000000003,33.369999999999997,34.64]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",28.62,28.54,28.62,28.54,29.02,29.02,29.02,29.42,27.86,27.86,28.54,28.54,28.54,29,29,28.46,28.54,29.02,28.62,29.42,29,27.86,28.46]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19]
["MT4","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07]
[null,"Cargo por Energía Activa",{"$nulls":4},"ctm.S/./kW.h",30.04,29.95,30.04,29.95,30.46,30.46,30.46,30.87,29.21,29.21,29.95,29.95,29.95,31.03,31.03,29.97,29.95,30.46,30.04,30.87,31.03,29.21,29.97]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27,65.27]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68,41.68]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55,24.55]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14,24.14]
[null,"Cargo por Energía Reactiva que Exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19]
["BAJA TENSION"]
["BT2","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27,14.27]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",37.35,37.22,37.35,37.22,37.9,37.9,37.9,38.35,36.21,36.21,37.22,37.22,37.22,40.450000000000003,40.450000000000003,37.590000000000003,37.22,37.9,37.35,38.35,40.450000000000003,36.21,37.590000000000003]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",31.05,30.97,31.05,30.97,31.49,31.49,31.49,31.93,30.23,30.23,30.97,30.97,30.97,31.47,31.47,30.88,30.97,31.49,31.05,31.93,31.47,30.23,30.88]
[null,"Cargo por Potencia Activa de Generación en HP",{"$nulls":4},"S/./kW-mes",73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994,73.959999999999994]
[null,"Cargo por Potencia Activa por uso de redes de Distribución en HP",{"$nulls":4},"S/./kW-mes",106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39,106.39]
[null,"Cargo por Exceso de Potencia Activa por uso de redes de Distribución en HFP",{"$nulls":4},"S/./kW-mes",78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995,78.239999999999995]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19]
["BT3","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",37.35,37.22,37.35,37.22,37.9,37.9,37.9,38.35,36.21,36.21,37.22,37.22,37.22,40.450000000000003,40.450000000000003,37.590000000000003,37.22,37.9,37.35,38.35,40.450000000000003,36.21,37.590000000000003]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",31.05,30.97,31.05,30.97,31.49,31.49,31.49,31.93,30.23,30.23,30.97,30.97,30.97,31.47,31.47,30.88,30.97,31.49,31.05,31.93,31.47,30.23,30.88]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19]
["BT4","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07]
[null,"Cargo por Energía Activa",{"$nulls":4},"ctm.S/./kW.h",32.590000000000003,32.5,32.590000000000003,32.5,33.049999999999997,33.049999999999997,33.049999999999997,33.51,31.7,31.7,32.5,32.5,32.5,33.67,33.67,32.53,32.5,33.049999999999997,32.590000000000003,33.51,33.67,31.7,32.53]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11,52.11]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15,50.15]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33,103.33]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44,100.44]
[null,"Cargo por Energía Reactiva que Exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19,5.19]
["BT5A","a) Usuarios con demanda maximia mensuakl de hasta 20KW en HP y HFP"]
[null,"Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",238.19,238.04,238.19,238.04,238.72,238.72,238.72,239.17,237.03,237.03,238.04,238.04,238.04,241.27,241.27,238.41,238.04,238.72,238.19,239.17,241.27,237.03,238.41]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",31.05,30.97,31.05,30.97,31.49,31.49,31.49,31.93,30.23,30.23,30.97,30.97,30.97,31.47,31.47,30.88,30.97,31.49,31.05,31.93,31.47,30.23,30.88]
[null,"Cargo por Exceso de Potencia en HFP",{"$nulls":4},"S/.kW-mes",96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65]
[null,"b) Usuarios con demanda maximia mensuakl de hasta 20KW en HP y 50KW en HFP"]
[null,"Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",282.55,282.39999999999998,282.55,282.39999999999998,283.08999999999997,283.08999999999997,283.08999999999997,283.52999999999997,281.39999999999998,281.39999999999998,282.39999999999998,282.39999999999998,282.39999999999998,285.63,285.63,282.77999999999997,282.39999999999998,283.08999999999997,282.55,283.52999999999997,285.63,281.39999999999998,282.77999999999997]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",31.05,30.97,31.05,30.97,31.49,31.49,31.49,31.93,30.23,30.23,30.97,30.97,30.97,31.47,31.47,30.88,30.97,31.49,31.05,31.93,31.47,30.23,30.88]
[null,"Cargo por Exceso de Potencia en HFP",{"$nulls":4},"S/.kW-mes",96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65,96.65]
["BT5B","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41]
[null,"           Cargo por energía activa",null,null,"   ",null,"ctm.S/./kW.h",60.16,40.11,40.11,40.11,60.16,40.11,40.11,40.11,60.16,40.11,60.16,40.11,40.11,60.16,40.11,60.16,40.11,40.11,40.11,40.11,40.11,40.11,40.11]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",18.05,12.03,12.03,12.03,18.05,12.03,12.03,12.03,18.05,12.03,18.05,12.03,12.03,18.05,12.03,18.05,12.03,12.03,12.03,12.03,12.03,12.03,12.03]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14]
[null,"c) No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",88.38,88.28,88.38,88.28,88.84,88.84,88.84,89.29,87.49,87.49,88.28,88.28,88.28,89.46,89.46,88.32,88.28,88.84,88.38,89.29,89.46,87.49,88.32]
["BT5C-AP","           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22,5.22]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",86.91,86.82,86.91,86.82,87.35,87.35,87.35,87.78,86.05,86.05,86.82,86.82,86.82,87.94,87.94,86.84,86.82,87.35,86.91,87.78,87.94,86.05,86.84]
["BT5D","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",45.11,30.03,30.07,30.03,45.41,30.28,30.28,30.48,44.5,29.67,45.04,30.03,30.03,45.83,30.55,45.05,30.03,30.28,30.07,30.48,30.55,29.67,30.04]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",13.53,9.01,9.02,9.01,13.62,9.08,9.08,9.14,13.35,8.9,13.51,9.01,9.01,13.75,9.17,13.52,9.01,9.08,9.02,9.14,9.17,8.9,9.01]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",60.14,60.05,60.14,60.05,60.55,60.55,60.55,60.95,59.33,59.33,60.05,60.05,60.05,61.1,61.1,60.07,60.05,60.55,60.14,60.95,61.1,59.33,60.07]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",63.09,62.99,63.09,62.99,63.52,63.52,63.52,63.94,62.24,62.24,62.99,62.99,62.99,64.09,64.09,63.01,62.99,63.52,63.09,63.94,64.09,62.24,63.01]
[null,"c)  No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",63.09,62.99,63.09,62.99,63.52,63.52,63.52,63.94,62.24,62.24,62.99,62.99,62.99,64.09,64.09,63.01,62.99,63.52,63.09,63.94,64.09,62.24,63.01]
["BT6","Cargo Fijo Mensual - Lectura Mensual",{"$nulls":4},"S/./mes",4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63,4.63]
[null,"Cargo por Potencia",{"$nulls":4},"cent. S/./W",33.409999999999997,33.369999999999997,33.409999999999997,33.369999999999997,33.58,33.58,33.58,33.75,33.06,33.06,33.369999999999997,33.369999999999997,33.369999999999997,33.82,33.82,33.380000000000003,33.369999999999997,33.58,33.409999999999997,33.75,33.82,33.06,33.380000000000003]
["BT7","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",60.16,40.11,40.11,40.11,60.16,40.11,40.11,40.11,60.16,40.11,60.16,40.11,40.11,60.16,40.11,60.16,40.11,40.11,40.11,40.11,40.11,40.11,40.11]
[null,"31-100 kWh"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53,3.53]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",18.05,12.03,12.03,12.03,18.05,12.03,12.03,12.03,18.05,12.03,18.05,12.03,12.03,18.05,12.03,18.05,12.03,12.03,12.03,12.03,12.03,12.03,12.03]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14]
[null,"c)  No Residencial"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7,3.7]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",87.08,86.98,87.08,86.98,87.54,87.54,87.54,87.98,86.2,86.2,86.98,86.98,86.98,88.14,88.14,87.01,86.98,87.54,87.08,87.98,88.14,86.2,87.01]
["BT5E","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",60.16,40.11,40.11,40.11,60.16,40.11,40.11,40.11,60.16,40.11,60.16,40.11,40.11,60.16,40.11,60.16,40.11,40.11,40.11,40.11,40.11,40.11,40.11]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77,2.77]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",18.05,12.03,12.03,12.03,18.05,12.03,12.03,12.03,18.05,12.03,18.05,12.03,12.03,18.05,12.03,18.05,12.03,12.03,12.03,12.03,12.03,12.03,12.03]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14]
[null,"c)  No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91,2.91]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",88.36,88.25,88.36,88.25,88.82,88.82,88.82,89.26,87.46,87.46,88.25,88.25,88.25,89.43,89.43,88.28,88.25,88.82,88.36,89.26,89.43,87.46,88.28]
["BT5F","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",60.16,40.11,40.11,40.11,60.16,40.11,40.11,40.11,60.16,40.11,60.16,40.11,40.11,60.16,40.11,60.16,40.11,40.11,40.11,40.11,40.11,40.11,40.11]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",45.73,30.45,30.49,30.45,46.04,30.7,30.7,30.91,45.14,30.1,45.67,30.45,30.45,46.03,30.69,45.61,30.45,30.7,30.49,30.91,30.69,30.1,30.41]
[null,"31-100 kWh"]
[null,"         Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46,4.46]
[null,"         Cargo por energía activa Hora Punta-Primeros 30 kWh",{"$nulls":4},"ctm.S/./kW.h",60.16,40.11,40.11,40.11,60.16,40.11,40.11,40.11,60.16,40.11,60.16,40.11,40.11,60.16,40.11,60.16,40.11,40.11,40.11,40.11,40.11,40.11,40.11]
[null,"         Cargo por energía activa Fuera de Punta-Primeros 30 kWh",{"$nulls":4},"ctm.S/./kW.h",45.73,30.45,30.49,30.45,46.04,30.7,30.7,30.91,45.14,30.1,45.67,30.45,30.45,46.03,30.69,45.61,30.45,30.7,30.49,30.91,30.69,30.1,30.41]
[null,"         Cargo por energía activa Hora Punta-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994,80.209999999999994]
[null,"         Cargo por energía activa Fuera de Punta-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",60.97,60.89,60.97,60.89,61.39,61.39,61.39,61.81,60.19,60.19,60.89,60.89,60.89,61.37,61.37,60.81,60.89,61.39,60.97,61.81,61.37,60.19,60.81]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68,4.68]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14,84.14]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",63.96,63.87,63.96,63.87,64.400000000000006,64.400000000000006,64.400000000000006,64.84,63.14,63.14,63.87,63.87,63.87,64.38,64.38,63.79,63.87,64.400000000000006,63.96,64.84,64.38,63.14,63.79]
[null,"c) No Residencial"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07,13.07]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",135.77000000000001,135.63999999999999,135.77000000000001,135.63999999999999,136.32,136.32,136.32,136.77000000000001,134.63,134.63,135.63999999999999,135.63999999999999,135.63999999999999,138.87,138.87,136,135.63999999999999,136.32,135.77000000000001,136.77000000000001,138.87,134.63,136]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",63.96,63.87,63.96,63.87,64.400000000000006,64.400000000000006,64.400000000000006,64.84,63.14,63.14,63.87,63.87,63.87,64.38,64.38,63.79,63.87,64.400000000000006,63.96,64.84,64.38,63.14,63.79]
["BT8","SUMINISTROS RURALES CON CELDAS FOTOVOLTAICAS (Sierra)",{"$nulls":5},"Inversion 100% Estado",{"$nulls":5},"Inversion 100% Empresa",{"$nulls":5},"  "]
[null,"Tipo de Módulo",{"$nulls":5},"BT8-070","BT8-100","BT8-160","BT8-240","BT8-320","BT8-050-Pre","BT8-070","BT8-100","BT8-160","BT8-240","BT8-320","BT8-050-Pre"]
[null,"Cargo Fijo Equivalente por Energia Promedio",{"$nulls":4},"ctm.S/./kW.h",98.24,76.349999999999994,60.1,44.35,67.55,130.85,150.71,117.45,91.45,69.239999999999995,106.54,167.97]

{"sheet":"CONEXION","index":1,"n_rows":131,"n_cols":11,"rows_kept":131,"cut":false,"hidden":false,"merged":[[0,0,0,10],[129,1,129,7],[109,3,109,4],[113,2,113,4],[115,0,115,1],[116,5,116,7],[128,1,128,7],[122,1,122,4],[114,0,114,1],[14,0,26,0],[36,3,36,4],[36,5,36,6],[40,3,40,4],[62,3,62,4],[67,5,67,6],[75,3,75,4],[75,5,75,6],[68,5,68,6],[115,5,115,7],[108,3,108,4],[112,5,112,7],[119,1,119,4],[110,5,110,7],[107,5,107,7],[109,5,109,7],[87,0,87,1],[87,3,87,4],[93,3,93,4],[92,3,92,4],[78,0,78,4],[4,5,4,6],[3,5,3,6],[32,5,32,6],[51,5,51,6],[49,5,49,6],[14,5,14,6],[22,5,22,6],[23,5,23,6],[9,5,9,6],[50,3,50,4],[50,5,50,6],[42,5,42,6],[92,5,92,7],[66,5,66,6],[24,3,24,4],[41,5,41,6],[24,5,24,6],[49,3,49,4],[87,5,87,7],[6,5,6,6],[10,5,10,6],[34,5,34,6],[43,5,43,6],[3,3,3,4],[11,5,11,6],[12,5,12,6],[25,3,25,4],[25,5,25,6],[31,3,31,4],[5,5,5,6],[8,5,8,6],[35,5,35,6],[17,5,17,6],[18,5,18,6],[51,3,51,4],[63,5,63,6],[53,3,53,4],[53,5,53,6],[88,5,88,7],[89,5,89,7],[90,5,90,7],[93,5,93,7],[95,5,95,7],[7,5,7,6],[52,3,52,4],[52,5,52,6],[57,3,57,4],[57,5,57,6],[58,3,58,4],[58,5,58,6],[62,5,62,6],[65,5,65,6],[19,5,19,6],[20,5,20,6],[21,5,21,6],[47,5,47,6],[64,5,64,6],[48,5,48,6],[44,5,44,6],[45,5,45,6],[46,5,46,6],[40,5,40,6],[97,5,97,7],[96,5,96,7],[108,5,108,7],[91,5,91,7],[94,5,94,7],[105,3,105,4],[100,5,100,7],[104,3,104,4],[104,5,104,7],[101,3,101,4],[100,3,100,4],[99,5,99,7],[102,3,102,4],[103,3,103,4],[101,5,101,7],[102,5,102,7],[103,5,103,7],[1,0,1,8],[4,0,13,0],[4,1,13,1],[4,2,9,2],[4,3,4,4],[36,1,37,1],[37,3,37,4],[37,5,37,6],[34,2,35,2],[34,3,34,4],[32,0,35,0],[32,1,35,1],[32,2,33,2],[32,3,32,4],[13,5,13,6],[15,5,15,6],[33,5,33,6],[31,5,31,6],[16,5,16,6],[26,3,26,4],[26,5,26,6],[14,1,21,1],[14,2,17,2],[14,3,14,4],[10,2,13,2],[10,3,10,4],[22,3,22,4],[41,2,44,2],[41,3,41,4],[36,0,37,0],[23,3,23,4],[23,1,26,1],[18,2,21,2],[18,3,18,4],[78,9,78,10],[76,3,76,4],[76,5,76,6],[67,3,67,4],[63,3,63,4],[58,0,59,0],[58,1,59,1],[59,3,59,4],[59,5,59,6],[74,3,74,4],[74,5,74,6],[78,5,78,6],[78,7,78,8],[130,1,130,7],[124,1,124,4],[116,0,116,1],[117,5,117,7],[114,2,114,4],[110,3,110,4],[104,0,104,1],[102,0,102,1],[97,3,97,4],[127,1,127,7],[121,1,121,4],[114,5,114,7],[113,0,113,1],[126,1,126,7],[120,1,120,4],[123,1,123,4],[107,3,107,4],[106,3,106,4],[106,5,106,7],[113,5,113,7],[111,5,111,7],[111,0,111,1],[105,5,105,7],[98,5,98,7],[45,2,48,2],[45,3,45,4],[41,0,53,0],[41,1,48,1],[94,0,94,1],[94,3,94,4],[90,3,90,4],[88,0,88,1],[88,3,88,4],[50,1,53,1]]}
[]
["PRESUPUESTOS DE LA CONEXIÓN ELECTRICA (NO INCLUYE IGV)"]
["Conexiones en Baja Tensión 220 V - Soles",{"$nulls":5},"Vigente a partir del 04-10-2022"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Aérea (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT5A",null,1156,1296]
[{"$nulls":5},"BT5B (2 hilos)",null,336,474]
[{"$nulls":5},"BT5B (2 hilos) - Rural (1)",null,386]
[{"$nulls":5},"BT5B (3 hilos)",null,343,483]
[{"$nulls":5},"BT5B (3 hilos) - Rural (1)",null,394]
[{"$nulls":5},"BT6",null,248,402]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT5A",null,1187,1304]
[{"$nulls":5},"BT5B (2 hilos)",null,368,483]
[{"$nulls":5},"BT5B (3 hilos)",null,374,491]
[{"$nulls":5},"BT6",null,279,408]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5A",null,2200,2337]
[{"$nulls":5},"BT5B",null,636,774]
[{"$nulls":5},"BT6",null,434,526]
[{"$nulls":5},"BT2/BT3/BT4",null,2760,2852]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5A",null,2232,2348]
[{"$nulls":5},"BT5B",null,668,783]
[{"$nulls":5},"BT6",null,466,537]
[{"$nulls":5},"BT2/BT3/BT4",null,2936,3007]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW",null,"BT5A/BT5B/BT2/BT3/BT4",null,3755,4076]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW",null,"BT2/BT3/BT4",null,4017,4882]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW",null,"BT2/BT3/BT4",null,null,6844]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW",null,"BT2/BT3/BT4",null,null,9020]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW",null,"BT2/BT3/BT4",null,null,9887]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.            (3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
[]
["Conexiones en Baja Tensión Múltiples 220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Conexión","Caja toma (1)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT5B (2 hilos)",null,196,86]
[{"$nulls":5},"BT5B (3 hilos)",null,202,86]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT5B (2 hilos)",null,213,153]
[{"$nulls":5},"BT5B (3 hilos)",null,220,153]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5B",null,408,154]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5B",null,435,315]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["Conexiones en Baja Tensión 380/220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                       Tarifaria",null,"Aérea            (1)","Subterránea (1)(2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5A",null,2251,2436]
[{"$nulls":5},"BT5B",null,642,829]
[{"$nulls":5},"BT6",null,442,578]
[{"$nulls":5},"BT2/BT3/BT4",null,2759,2895]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5A",null,2254,2441]
[{"$nulls":5},"BT5B",null,646,833]
[{"$nulls":5},"BT6",null,445,582]
[{"$nulls":5},"BT2/BT3/BT4",null,2762,2900]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW",null,"BT5A/BT5B/BT2/BT3/BT4",null,3546,3898]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW",null,"BT2/BT3/BT4",null,3799,4283]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW",null,"BT2/BT3/BT4",null,null,5523]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW",null,"BT2/BT3/BT4",null,null,7729]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW",null,"BT2/BT3/BT4",null,null,8470]
["(1) Aplicable a conexiones con acometida simple o doble."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 380/220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Conexión","Caja Toma (1)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5B",null,406,128]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5B",null,410,284]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["Conexiones en Baja Tensión 220 V - Prepago - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Aérea            (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT7 (2 hilos)",null,729,870]
[{"$nulls":5},"BT7 (2 hilos) - Rural (1)",null,780]
[{"$nulls":5},"BT7 (3 hilos)",null,1015,874]
[{"$nulls":5},"BT7 (3 hilos) - Rural (1)",null,1065]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT7 (2 hilos)",null,760,876]
[{"$nulls":5},"BT7 (3 hilos)",null,1047,892]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble."]
["(3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
[]
["Costo por Metro de Cable de Conexiones en Baja Tensión 220 V - Prepago - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Costo"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT7",null,6]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT7",null,7]
[]
["Conexiones Básicas en Media Tensión - Soles",{"$nulls":4},"10 kV",null,"13.2/7.62 kV",null,"20 kV - 22.9/13.2 kV"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","PMI","Celda","PMI","Celda","PMI","Celda"]
["Trifásica","C5","C5.1","Pc ≤ 100 kW","MT2/MT3/MT4",11860,20270,14550,26480,16362,26518]
[null,null,"C5.2","100 kW < Pc ≤ 400 kW","MT2/MT3/MT4",15861,18236,14637,23775,16362,26518]
[null,null,"C5.3","400 kW < Pc ≤ 700 kW","MT2/MT3/MT4",14244,17434,15044,22710,17162,29679]
[null,null,"C5.4","700 kW < Pc ≤ 1000 kW","MT2/MT3/MT4",14710,16560,15044,22710,17541,28953]
[null,null,"C5.5","1000 kW < Pc ≤ 2500 kW","MT2/MT3/MT4",17963,17319,16405,22356,19240,26939]
[]
["Otros Elementos Electromecánicos en Media Tensión - Soles"]
["Elemento",null,"Tipo de red","Potencia Conectada (Pc)",null,"Descripción",null,null,"10 kV","13.2/7.62 kV","20 kV - 22.9/13.2 kV"]
["Empalme de acometida",null,"Aérea","Pc ≤ 1000 kW",null,"A red aérea con cable autoportante",null,null,1347,1167,1117]
[{"$nulls":5},"A red aérea con conductor desnudo",null,null,207,207,207]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"A red aérea con cable autoportante",null,null,1347,1167,1117]
[{"$nulls":5},"A red aérea con conductor desnudo",null,null,207,207,207]
[null,null,"Subterránea","Pc ≤ 1000 kW",null,"A red subterránea",null,null,7631,7631,7631]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"A red subterránea",null,null,7631,7631,7631]
["Cable de acometida",null,"Aérea","Pc ≤ 1000 kW",null,"Con cable autoportante y salida a red subterránea",null,null,7985,7626,7742]
[{"$nulls":5},"Con conductor desnudo y salida a red aérea",null,null,6493,6506,6855]
[{"$nulls":5},"Con conductor desnudo y salida a red subterránea",null,null,6646,6479,6520]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con cable autoportante y salida a red subterránea",null,null,8423,7626,7742]
[{"$nulls":5},"Con conductor desnudo y salida a red aérea",null,null,7488,6563,6855]
[{"$nulls":5},"Con conductor desnudo y salida a red subterránea",null,null,7330,6536,6520]
[null,null,"Subterránea-Aérea","Pc ≤ 1000 kW",null,"Con conductor desnudo y salida a red subterránea",null,null,7708,7349,8173]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con conductor desnudo y salida a red subterránea",null,null,8329,7349,8173]
["Caja de protección",null,"Subterránea","Pc ≤ 1000 kW",null,"Para celda interior",null,null,7475,7198,7446]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Para celda interior",null,null,7475,7198,7446]
["Sistema de protección y seccionamiento",null,"Aérea","Pc ≤ 100 kW",null,"Con seccionador cut-out",null,null,1795,1681,1890]
[null,null,null,"100 kW < Pc ≤ 400 kW",null,"Con seccionador cut-out",null,null,1800,1676,1892]
[null,null,null,"400 kW < Pc ≤ 700 kW",null,"Con seccionador cut-out",null,null,1823,1695,1892]
[null,null,null,"700 kW < Pc ≤ 1000 kW",null,"Con seccionador cut-out",null,null,1862,1713,1896]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con seccionador cut-out",null,null,7778,6930,7443]
[null,null,"Subterránea","Pc ≤ 1000 kW",null,"Con seccionador de potencia para celda interior",null,null,20452,21417,27462]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con seccionador de potencia para celda interior",null,null,32812,33887,27317]
["Protección sobretensión",null,"Aérea",null,null,"Para instalación exterior",null,null,1084,1154,1457]
[null,null,"Subterránea",null,null,"Para instalación interior",null,null,1723,2086,2355]
["Zanja (metro lineal)",null,"Aérea/Subterránea",null,null,"Para PMI o celda interior",null,null,66,66,66]
["Rotura y reparación de vereda (m2)",null,"Aérea/Subterránea",null,null,"Para PMI o celda interior",null,null,160,160,160]
["Murete",null,"Aérea",null,null,"Para PMI",null,null,342,342,342]
["Protección de estructuras",null,"Aérea",null,null,"Bloque de concreto",null,null,582,582,582]
[{"$nulls":5},"Riel de acero",null,null,189,189,189]
[null,"Costo por Vereda, Murete y Mástil en Baja Tensión - Soles"]
[null,"Descripción",null,null,null,"Unidad","Costo"]
[null,"Rotura y resane de vereda en baja tensión",null,null,null,"m2",160]
[null,"Murete baja tensión, conexión monofásica",null,null,null,"Unidad",197]
[null,"Murete baja tensión, conexión trifásica",null,null,null,"Unidad",218]
[null,"Mástil metálico de 3 m",null,null,null,"Unidad",99]
[null,"Mástil metálico de 6 m",null,null,null,"Unidad",156]
[null,"Costos Adicionales al Sistema de Proteccion y Seccionamiento - Soles"]
[null,"Descripción",{"$nulls":6},"Unidad","Costo"]
[null,"Seccionador Tipo Expulsión, Exterior, Unipolar, Bajo Carga, 10kV, 300A x 3 (1)",{"$nulls":6},"Unidad",2335]
[null,"Seccionador Tipo Expulsión, Exterior, Unipolar, Bajo Carga, 22.9kV, 200A x 3 (1)",{"$nulls":6},"Unidad",3873]
[null,"Seccionador Bajo Carga, Interior, Tripolar, 10kV, 400A x 1 (2)",{"$nulls":6},"Unidad",6382]
[null,"Aislador Extensor, Polimerico, 25kv, Para Cut-Out x 3 (3)",{"$nulls":6},"Unidad",895]

{"sheet":"REP_MTTO","index":2,"n_rows":95,"n_cols":15,"rows_kept":95,"cut":false,"hidden":false,"merged":[[1,0,1,14],[5,0,14,0],[5,1,14,1],[5,2,10,2],[5,3,10,3],[62,11,62,12],[3,7,3,8],[3,9,3,10],[3,11,3,12],[3,13,3,14],[54,8,54,14],[43,7,43,8],[43,9,43,10],[43,11,43,12],[43,13,43,14],[32,0,32,4],[32,5,32,6],[32,7,32,8],[32,9,32,10],[32,11,32,12],[15,0,28,0],[15,1,22,1],[15,2,18,2],[11,2,14,2],[11,3,14,3],[25,1,28,1],[19,2,22,2],[19,3,22,3],[15,3,18,3],[81,0,85,0],[81,1,85,1],[70,1,75,1],[70,2,73,2],[74,2,75,2],[79,0,79,4],[62,5,62,6],[62,7,62,8],[62,9,62,10],[79,5,79,6],[79,7,79,8],[79,9,79,10]]}
[]
["CARGOS DE REPOSICION Y MANTENIMIENTO  DE LA CONEXIÓN ELECTRICA (NO INCLUYE IGV)"]
["Conexiones en Baja Tensión 220 V - Nuevos Soles",{"$nulls":6},"Vigente a partir del 04-10-2022"]
[{"$nulls":7},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT5A",1.81,1.83]
[{"$nulls":4},"BT5B (2 hilos)",null,null,1.32,1.33,1.38,1.3900000000000001,1.58,1.5899999999999999,1.64,1.65]
[{"$nulls":4},"BT5B (2 hilos) - Rural (1)",null,null,1.53,null,1.6,null,1.85,null,1.92]
[{"$nulls":4},"BT5B (3 hilos)",null,null,1.32,1.33,1.38,1.3900000000000001,1.58,1.5899999999999999,1.64,1.65]
[{"$nulls":4},"BT5B (3 hilos) - Rural (1)",null,null,1.58,null,1.6500000000000001,null,1.9000000000000001,null,1.97]
[{"$nulls":4},"BT6",0.77,0.77999999999999992]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT5A",1.8599999999999999,1.83]
[{"$nulls":4},"BT5B (2 hilos)",null,null,1.32,1.33,1.38,1.3900000000000001,1.58,1.5899999999999999,1.64,1.65]
[{"$nulls":4},"BT5B (3 hilos)",null,null,1.32,1.33,1.38,1.3900000000000001,1.58,1.5899999999999999,1.64,1.65]
[{"$nulls":4},"BT6",0.77,0.77999999999999992]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5A",3.43,3.48]
[{"$nulls":4},"BT5B",null,null,1.82,1.88,1.82,1.88,1.97,2.0100000000000002,1.97,2.0100000000000002]
[{"$nulls":4},"BT6",0.84000000000000008,0.84]
[{"$nulls":4},"BT2/BT3/BT4",4,4.0599999999999996]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5A",3.43,3.48]
[{"$nulls":4},"BT5B",null,null,1.82,1.88,1.82,1.88,1.97,2.0100000000000002,1.97,2.0100000000000002]
[{"$nulls":4},"BT6",0.84000000000000008,0.84]
[{"$nulls":4},"BT2/BT3/BT4",4.05,4.1099999999999994]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW","BT5B",5.5299999999999994,5.49]
[{"$nulls":4},"BT5A/BT2/BT3/BT4",5.5299999999999994,5.49]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW","BT2/BT3/BT4",5.6099999999999994,5.75]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW","BT2/BT3/BT4",null,6.3900000000000006]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW","BT2/BT3/BT4",null,7.1]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW","BT2/BT3/BT4",null,7.3599999999999994]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.            (3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 220 V - Nuevos Soles"]
[{"$nulls":5},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT5B (2 hilos)",1.37,1.26,1.43,1.32,1.6300000000000001,1.52,1.69,1.58]
[{"$nulls":4},"BT5B (3 hilos)",1.4000000000000001,1.29,1.46,1.35,1.6600000000000001,1.55,1.72,1.61]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT5B (2 hilos)",1.4000000000000001,1.29,1.46,1.35,1.6600000000000001,1.55,1.72,1.61]
[{"$nulls":4},"BT5B (3 hilos)",1.4000000000000001,1.29,1.46,1.35,1.6600000000000001,1.55,1.72,1.61]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5B",1.8599999999999999,1.7999999999999998,1.8599999999999999,1.7999999999999998,2.0099999999999998,1.9300000000000002,2.0099999999999998,1.9300000000000002]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5B",1.9100000000000001,1.85,1.9100000000000001,1.85,2.06,1.98,2.06,1.98]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión 380/220 V - Nuevos Soles"]
[{"$nulls":7},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5A",3.43,3.48]
[{"$nulls":4},"BT5B",null,null,1.82,1.92,1.82,1.92,1.97,2.0499999999999998,1.97,2.0499999999999998]
[{"$nulls":4},"BT6",0.84000000000000008,0.8899999999999999]
[{"$nulls":4},"BT2/BT3/BT4",4,4.0599999999999996]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5A",3.43,3.48]
[{"$nulls":4},"BT5B",null,null,1.82,1.92,1.82,1.92,1.97,2.0499999999999998,1.97,2.0499999999999998]
[{"$nulls":4},"BT6",0.84000000000000008,0.8899999999999999]
[{"$nulls":4},"BT2/BT3/BT4",4,4.0599999999999996]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW","BT5B",5.4799999999999995,5.4]
[{"$nulls":4},"BT5A/BT2/BT3/BT4",5.4799999999999995,5.4]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW","BT2/BT3/BT4",5.57,5.53]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW","BT2/BT3/BT4",null,5.97]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW","BT2/BT3/BT4",null,6.67]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW","BT2/BT3/BT4",null,6.92]
["(1) Aplicable a conexiones con acometida simple o doble."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 380/220 V - Nuevos Soles"]
[{"$nulls":5},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5B",1.8599999999999999,1.7999999999999998,1.8599999999999999,1.7999999999999998,2.0099999999999998,1.9300000000000002,2.0099999999999998,1.9300000000000002]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5B",1.9100000000000001,1.85,1.9100000000000001,1.85,2.06,1.98,2.06,1.98]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión 220 V - Prepago - Nuevos Soles"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea              (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT7 (2 hilos)",1.9,1.93]
[{"$nulls":4},"BT7 (2 hilos) - Rural (1)",1.9,0.76]
[{"$nulls":4},"BT7 (3 hilos)",2.4900000000000002,2.42]
[{"$nulls":4},"BT7 (3 hilos) - Rural (1)",2.5299999999999998,0.76]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT7 (2 hilos)",1.9,1.93]
[{"$nulls":4},"BT7 (3 hilos)",2.4900000000000002,2.42]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.",null,null,null,"(3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Media Tensión - Nuevos Soles"]
[{"$nulls":5},"10 kV",null,"13.2/7.62 kV",null,"20 kV - 22.9/13.2 kV"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","PMI","Celda","PMI","Celda","PMI","Celda"]
["Trifásica","C5","C5.1","Pc ≤ 100 kW","MT2/MT3/MT4",19.63,28.23,20.420000000000002,30.560000000000002,21.759999999999998,33.409999999999997]
[null,null,"C5.2","100 kW < Pc ≤ 400 kW","MT2/MT3/MT4",20.95,27.55,20.47,29.68,21.759999999999998,33.409999999999997]
[null,null,"C5.3","400 kW < Pc ≤ 700 kW","MT2/MT3/MT4",20.420000000000002,27.3,20.59,29.36,22.05,34.450000000000003]
[null,null,"C5.4","700 kW < Pc ≤ 1000 kW","MT2/MT3/MT4",20.54,27.03,20.59,29.36,22.17,34.21]
[null,null,"C5.5","1000 kW < Pc ≤ 2500 kW","MT2/MT3/MT4",22.22,28.14,21.61,30.12,23.56,34.150000000000006]
{"$rows_empty":8}
["  "]

{"sheet":"COR_RECONEX","index":3,"n_rows":113,"n_cols":6,"rows_kept":113,"cut":false,"hidden":false,"merged":[[112,0,112,1],[110,0,110,1],[111,0,111,1],[98,0,98,3],[98,4,98,5],[82,4,82,5],[56,0,61,0],[58,1,59,1],[60,1,61,1],[64,0,64,3],[64,4,64,5],[45,4,45,5],[47,0,52,0],[50,1,52,1],[36,0,43,0],[36,1,39,1],[40,1,43,1],[47,1,49,1],[54,4,54,5],[6,0,13,0],[6,1,9,1],[10,1,13,1],[0,0,0,5],[1,0,1,5],[4,0,4,2],[4,3,5,3],[26,0,31,0],[28,1,29,1],[30,1,31,1],[15,4,15,5],[17,0,22,0],[20,1,22,1],[17,1,19,1],[24,0,24,3],[84,0,95,0],[100,0,107,0],[34,0,34,2],[34,3,35,3],[45,0,45,3],[54,0,54,3],[66,0,79,0],[82,0,82,3]]}
[]
["IMPORTES MAXIMOS DE CORTE Y RECONEXION (NO INCLUYE IGV)"]
["Conexiones monofásicas, hasta 10 kW, BT5A, BT5B y BT6"]
[null,null,"Vigente a partir del 04-10-2022"]
["Descripción",null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Fusible o interruptor (tapa sin ranura)",7.76]
[null,null,"Interruptor (tapa con ranura)",10.52]
[null,null,"Caja de medición (aislamiento acometida)",11.29]
[null,null,"Línea aérea (empalme)",27]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)",9.35]
[null,null,"Interruptor (tapa con ranura)",12.09]
[null,null,"Caja de medición (aislamiento acometida)",12.97]
[null,null,"Línea aérea (empalme)",32.799999999999997]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Retiro","RT conexión aérea","Camioneta",54.24,58.16]
[null,null,"RT conexión subterránea","Camioneta",55.24,58.95]
[null,null,"RT conexión mixta","Camioneta",55.24,58.95]
[null,"Reinstalación","RIconexión aérea","Camioneta",95.87,103.27]
[null,null,"RI conexión subterránea","Camioneta",72,77.86]
[null,null,"RI conexión mixta","Camioneta",72,77.86]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Caja de medición (aislamiento acometida bloqueada)","Camioneta",24.92,29.1]
[null,"Reconexión","Caja de medición (aislamiento acometida bloqueada)","Camioneta",22.5,27.64]
[null,"Retiro","RT conexión subterránea (empalme y cable de acometida)","Camioneta",184.98,192.38]
[null,null,"RT conexión mixta (empalme y cable de acometida)","Camioneta",184.98,192.38]
[null,"Reinstalación","RI conexión subterránea (empalme y cable de acometida)","Camioneta",255.21,265.08999999999997]
[null,null,"RI conexión mixta (empalme y cable de acometida)","Camioneta",255.21,265.08999999999997]
[]
["Conexiones Trifásicas, hasta 20 kW, BT5A, BT5B y BT6"]
["Descripción",null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Fusible o interruptor (tapa sin ranura)",9.2200000000000006]
[null,null,"Interruptor (tapa con ranura)",11.72]
[null,null,"Caja de medición (aislamiento acometida)",11.83]
[null,null,"Línea aérea (empalme)",26.73]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)",12.39]
[null,null,"Interruptor (tapa con ranura)",14.44]
[null,null,"Caja de medición (aislamiento acometida)",15.47]
[null,null,"Línea aérea (empalme)",33.729999999999997]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Retiro","RT conexión aérea","Camioneta",64.52,69.459999999999994]
[null,null,"RT conexión subterránea","Camioneta",59.95,63.64]
[null,null,"RT conexión mixta","Camioneta",59.95,63.64]
[null,"Reinstalación","RI conexión aérea","Camioneta",110.64,119.08]
[null,null,"RI conexión subterránea","Camioneta",80.78,87.35]
[null,null,"RI conexión mixta","Camioneta",80.78,87.35]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Caja de medición (aislamiento acometida bloqueada)","Camioneta",28.26,33.200000000000003]
[null,"Reconexión","Caja de medición (aislamiento acometida bloqueada)","Camioneta",30.44,34.29]
[null,"Retiro","RT conexión subterránea (empalme y cable de acometida)","Camioneta",203,210.4]
[null,null,"RT conexión mixta (empalme y cable de acometida)","Camioneta",203,210.4]
[null,"Reinstalación","RI conexión subterránea (empalme y cable de acometida)","Camioneta",298.04000000000002,298.04000000000002]
[null,null,"RI conexión mixta (empalme y cable de acometida)","Camioneta",288.2,296.86]
[]
["Conexiones Trifásicas, hasta 20 kW, resto de opciones (BT2,BT3 y BT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW resto de opciones (BT2,BT3 y BT4)","Corte","Fusible o interruptor (tapa sin ranura)","Camioneta",26.05,28.14]
[null,null,"Interruptor (tapa con ranura)","Camioneta",29.14,31.53]
[null,null,"Caja de medición (aislamiento acometida)","Camioneta",29.31,31.65]
[null,null,"Línea aérea (empalme)","Camioneta",41.73,44.69]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)","Camioneta",42.32,44.61]
[null,null,"Interruptor (tapa con ranura)","Camioneta",32.950000000000003,35.659999999999997]
[null,null,"Caja de medición (aislamiento acometida)","Camioneta",46.24,48.33]
[null,null,"Línea aérea (empalme)","Camioneta",62.64,65.73]
[null,"Retiro","RT conexión aérea","Camioneta",64.52,69.459999999999994]
[null,null,"RT conexión subterránea","Camioneta",59.95,63.64]
[null,null,"RT conexión mixta","Camioneta",59.95,63.64]
[null,"Reinstalación","RIconexión aérea","Camioneta",123.26,131.71]
[null,null,"RIión subterránea","Camioneta",93.41,100.02]
[null,null,"RI conexión mixta","Camioneta",93.41,100.02]
[]
["Conexiones trifásicas mayor a 20 kW, resto de opciones (BT2,BT3 y BT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica mayor a 20 kW resto de opciones (BT2,BT3 y BT4)","Corte","En fusible o interruptor (tapa sin ranura)","Camioneta",29.05,31.41]
[null,null,"En caja de medición (aislamiento acometida)","Camioneta",31.78,34.33]
[null,null,"En línea aérea (empalme)","Camioneta",47.21,50.39]
[null,"Reconexión","En fusible o interruptor (tapa sin ranura)","Camioneta",38.090000000000003,40.43]
[null,null,"En caja de medición (aislamiento acometida)","Camioneta",47.66,50.76]
[null,null,"En línea aérea (empalme)","Camioneta",76.31,80.53]
[null,"Retiro","En conexión aérea","Camioneta",94.08,101.43]
[null,null,"En conexión subterránea","Camioneta",88.1,94.66]
[null,null,"En conexión mixta","Camioneta",88.1,94.66]
[null,"Reinstalación","En conexión aérea","Camioneta",140.69,150.52000000000001]
[null,null,"En conexión subterránea","Camioneta",113.43,121.88]
[null,null,"En conexión mixta","Camioneta",113.43,121.88]
[]
["Conexiones trifásicas, hasta 2500 kW, resto de opciones (MT2,MT3 y MT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 2500 kW resto de opciones (MT2,MT3 y MT4)","Corte","En sistema de protección - PMI","Camioneta",59.21,64.13]
[null,null,"En sistema de protección - Celda","Camioneta",59.16,64.06]
[null,"Reconexión","En sistema de protección - PMI","Camioneta",59.16,64.06]
[null,null,"En sistema de protección - Celda","Camioneta",71,76.849999999999994]
[null,"Retiro","En sistema de protección - PMI","Camioneta",249.57,259.39999999999998]
[null,null,"En sistema de protección - Celda","Camioneta",101.36,109.79]
[null,"Reinstalación","En sistema de protección - PMI","Camioneta",441.74,453.57]
[null,null,"En sistema de protección - Celda","Camioneta",260.49,270.36]
[]
["Suministros Rurales con Celdas Fotovoltaicas (Sierra)"]
["Tipo",null,"Costo Total (S/.)"]
["Corte",null,8.57]
["Reconexión",null,10.68]