{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["ENERGIA","CONEXION","REP_MTTO","COR_RECONEX"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ENERGIA","index":0,"n_rows":150,"n_cols":30,"rows_kept":150,"cut":false,"hidden":false,"merged":[[1,0,1,1],[2,0,2,5],[147,7,147,12],[147,13,147,18]]}
["PLIEGO TARIFARIO DEL SERVICIO PUBLICO DE ELECTRICIDAD (SIN IGV)"]
["2022-06-04",{"$nulls":14},"VIGENTE A PARTIR DEL DIA 04-06-2022-R"]
["SISTEMA ELECTRICO",{"$nulls":6},"Cusco","Valle Sagrado 1","Valle Sagrado 2","Valle Sagrado 3","Sicuani","Sicuani Rural","Combapata-Chumbivilcas","Yauri","La Convención Macupicchu","La Convención Rural","Abancay","Abancay Rural-Chuquibambilla-Chacapuente","Andahuyalas","Puerto Maldonado","Puerto Maldonad Rural, Iñapari, Iberia","Mazuco","SER-Apurimac y Valle Sagrado","SER-Valle Vilcanota","SER-Quispicanchis","SER-Espinar","SER-Iberia","SER-Machupicchu","SER-Mazuco"]
[]
["MEDIA TENSION",{"$nulls":5},"UNIDAD",{"$nulls":10},"TARIFA"]
["MT2","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",33.44,33.32,33.44,33.32,33.909999999999997,33.909999999999997,33.909999999999997,34.299999999999997,32.450000000000003,32.450000000000003,33.32,33.32,33.32,36.130000000000003,36.130000000000003,33.630000000000003,33.32,33.909999999999997,33.44,34.299999999999997,36.130000000000003,32.450000000000003,33.630000000000003]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",27.98,27.91,27.98,27.91,28.36,28.36,28.36,28.75,27.28,27.28,27.91,27.91,27.91,28.35,28.35,27.85,27.91,28.36,27.98,28.75,28.35,27.28,27.85]
[null,"Cargo por Potencia Activa de Generación en HP",{"$nulls":4},"S/./kW-mes",65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006,65.900000000000006]
[null,"Cargo por Potencia Activa por uso de redes de Distribución en HP",{"$nulls":4},"S/./kW-mes",22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11,22.11]
[null,"Cargo por Exceso de Potencia Activa por uso de redes de Distribución en HFP",{"$nulls":4},"S/./kW-mes",22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64,22.64]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84]
["MT3","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",33.44,33.32,33.44,33.32,33.909999999999997,33.909999999999997,33.909999999999997,34.299999999999997,32.450000000000003,32.450000000000003,33.32,33.32,33.32,36.130000000000003,36.130000000000003,33.630000000000003,33.32,33.909999999999997,33.44,34.299999999999997,36.130000000000003,32.450000000000003,33.630000000000003]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",27.98,27.91,27.98,27.91,28.36,28.36,28.36,28.75,27.28,27.28,27.91,27.91,27.91,28.35,28.35,27.85,27.91,28.36,27.98,28.75,28.35,27.28,27.85]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84]
["MT4","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79]
[null,"Cargo por Energía Activa",{"$nulls":4},"ctm.S/./kW.h",29.32,29.24,29.32,29.24,29.73,29.73,29.73,30.12,28.54,28.54,29.24,29.24,29.24,30.26,30.26,29.27,29.24,29.73,29.32,30.12,30.26,28.54,29.27]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17,60.17]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69,23.69]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29,23.29]
[null,"Cargo por Energía Reactiva que Exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84]
["BAJA TENSION"]
["BT2","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95,13.95]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",36.299999999999997,36.15,36.299999999999997,36.15,36.799999999999997,36.799999999999997,36.799999999999997,37.22,35.200000000000003,35.200000000000003,36.15,36.15,36.15,39.200000000000003,39.200000000000003,36.49,36.15,36.799999999999997,36.299999999999997,37.22,39.200000000000003,35.200000000000003,36.49]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",30.36,30.28,30.36,30.28,30.78,30.78,30.78,31.21,29.6,29.6,30.28,30.28,30.28,30.77,30.77,30.21,30.28,30.78,30.36,31.21,30.77,29.6,30.21]
[null,"Cargo por Potencia Activa de Generación en HP",{"$nulls":4},"S/./kW-mes",68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19,68.19]
[null,"Cargo por Potencia Activa por uso de redes de Distribución en HP",{"$nulls":4},"S/./kW-mes",103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01,103.01]
[null,"Cargo por Exceso de Potencia Activa por uso de redes de Distribución en HFP",{"$nulls":4},"S/./kW-mes",75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83,75.83]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84]
["BT3","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",36.299999999999997,36.15,36.299999999999997,36.15,36.799999999999997,36.799999999999997,36.799999999999997,37.22,35.200000000000003,35.200000000000003,36.15,36.15,36.15,39.200000000000003,39.200000000000003,36.49,36.15,36.799999999999997,36.299999999999997,37.22,39.200000000000003,35.200000000000003,36.49]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",30.36,30.28,30.36,30.28,30.78,30.78,30.78,31.21,29.6,29.6,30.28,30.28,30.28,30.77,30.77,30.21,30.28,30.78,30.36,31.21,30.77,29.6,30.21]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84]
["BT4","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79]
[null,"Cargo por Energía Activa",{"$nulls":4},"ctm.S/./kW.h",31.82,31.72,31.82,31.72,32.26,32.26,32.26,32.68,30.98,30.98,31.72,31.72,31.72,32.83,32.83,31.75,31.72,32.26,31.82,32.68,32.83,30.98,31.75]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03,48.03]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23,46.23]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09,100.09]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28,97.28]
[null,"Cargo por Energía Reactiva que Exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84,4.84]
["BT5A","a) Usuarios con demanda maximia mensuakl de hasta 20KW en HP y HFP"]
[null,"Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",226.91,226.76,226.91,226.76,227.42,227.42,227.42,227.84,225.83,225.83,226.76,226.76,226.76,229.81,229.81,227.12,226.76,227.42,226.91,227.84,229.81,225.83,227.12]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",30.36,30.28,30.36,30.28,30.78,30.78,30.78,31.21,29.6,29.6,30.28,30.28,30.28,30.77,30.77,30.21,30.28,30.78,30.36,31.21,30.77,29.6,30.21]
[null,"Cargo por Exceso de Potencia en HFP",{"$nulls":4},"S/.kW-mes",93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69]
[null,"b) Usuarios con demanda maximia mensuakl de hasta 20KW en HP y 50KW en HFP"]
[null,"Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",269.02999999999997,268.88,269.02999999999997,268.88,269.52999999999997,269.52999999999997,269.52999999999997,269.95,267.94,267.94,268.88,268.88,268.88,271.93,271.93,269.23,268.88,269.52999999999997,269.02999999999997,269.95,271.93,267.94,269.23]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",30.36,30.28,30.36,30.28,30.78,30.78,30.78,31.21,29.6,29.6,30.28,30.28,30.28,30.77,30.77,30.21,30.28,30.78,30.36,31.21,30.77,29.6,30.21]
[null,"Cargo por Exceso de Potencia en HFP",{"$nulls":4},"S/.kW-mes",93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69,93.69]
["BT5B","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996]
[null,"           Cargo por energía activa",null,null,"   ",null,"ctm.S/./kW.h",59.24,39.5,39.5,39.5,59.24,39.5,39.5,39.5,59.24,39.5,59.24,39.5,39.5,59.24,39.5,59.24,39.5,39.5,39.5,39.5,39.5,39.5,39.5]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",17.77,11.85,11.85,11.85,17.77,11.85,11.85,11.85,17.77,11.85,17.77,11.85,11.85,17.77,11.85,17.77,11.85,11.85,11.85,11.85,11.85,11.85,11.85]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86]
[null,"c) No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",84.76,84.68,84.76,84.68,85.21,85.21,85.21,85.63,83.92,83.92,84.68,84.68,84.68,85.79,85.79,84.71,84.68,85.21,84.76,85.63,85.79,83.92,84.71]
["BT5C-AP","           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003,5.1100000000000003]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",83.33,83.24,83.33,83.24,83.75,83.75,83.75,84.15,82.53,82.53,83.24,83.24,83.24,84.3,84.3,83.27,83.24,83.75,83.33,84.15,84.3,82.53,83.27]
["BT5D","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",43.08,28.68,28.72,28.68,43.38,28.92,28.92,29.11,42.52,28.35,43.02,28.68,28.68,43.77,29.18,43.04,28.68,28.92,28.72,29.11,29.18,28.35,28.7]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996,4.3099999999999996]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",12.92,8.6,8.6199999999999992,8.6,13.01,8.68,8.68,8.73,12.76,8.5,12.91,8.6,8.6,13.13,8.75,12.91,8.6,8.68,8.6199999999999992,8.73,8.75,8.5,8.61]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",57.44,57.36,57.44,57.36,57.84,57.84,57.84,58.22,56.69,56.69,57.36,57.36,57.36,58.36,58.36,57.39,57.36,57.84,57.44,58.22,58.36,56.69,57.39]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",60.25,60.17,60.25,60.17,60.67,60.67,60.67,61.07,59.47,59.47,60.17,60.17,60.17,61.22,61.22,60.2,60.17,60.67,60.25,61.07,61.22,59.47,60.2]
[null,"c)  No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",60.25,60.17,60.25,60.17,60.67,60.67,60.67,61.07,59.47,59.47,60.17,60.17,60.17,61.22,61.22,60.2,60.17,60.67,60.25,61.07,61.22,59.47,60.2]
["BT6","Cargo Fijo Mensual - Lectura Mensual",{"$nulls":4},"S/./mes",4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996,4.5199999999999996]
[null,"Cargo por Potencia",{"$nulls":4},"cent. S/./W",32.04,32,32.04,32,32.200000000000003,32.200000000000003,32.200000000000003,32.369999999999997,31.72,31.72,32,32,32,32.42,32.42,32.020000000000003,32,32.200000000000003,32.04,32.369999999999997,32.42,31.72,32.020000000000003]
["BT7","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",59.24,39.5,39.5,39.5,59.24,39.5,39.5,39.5,59.12,39.42,59.24,39.5,39.5,59.24,39.5,59.24,39.5,39.5,39.5,39.5,39.5,39.42,39.5]
[null,"31-100 kWh"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46,3.46]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",17.77,11.85,11.85,11.85,17.77,11.85,11.85,11.85,17.739999999999998,11.82,17.77,11.85,11.85,17.77,11.85,17.77,11.85,11.85,11.85,11.85,11.85,11.82,11.85]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.83,78.83,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.83,78.989999999999995]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.69,82.69,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.69,82.86]
[null,"c)  No Residencial"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63,3.63]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",83.52,83.43,83.52,83.43,83.95,83.95,83.95,84.37,82.69,82.69,83.43,83.43,83.43,84.53,84.53,83.46,83.43,83.95,83.52,84.37,84.53,82.69,83.46]
["BT5E","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",59.24,39.5,39.5,39.5,59.24,39.5,39.5,39.5,59.24,39.5,59.24,39.5,39.5,59.24,39.5,59.24,39.5,39.5,39.5,39.5,39.5,39.5,39.5]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71,2.71]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",17.77,11.85,11.85,11.85,17.77,11.85,11.85,11.85,17.77,11.85,17.77,11.85,11.85,17.77,11.85,17.77,11.85,11.85,11.85,11.85,11.85,11.85,11.85]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86]
[null,"c)  No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84,2.84]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",84.74,84.65,84.74,84.65,85.18,85.18,85.18,85.61,83.9,83.9,84.65,84.65,84.65,85.76,85.76,84.69,84.65,85.18,84.74,85.61,85.76,83.9,84.69]
["BT5F","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",59.24,39.5,39.5,39.5,59.24,39.5,39.5,39.5,59.24,39.5,59.24,39.5,39.5,59.24,39.5,59.24,39.5,39.5,39.5,39.5,39.5,39.5,39.5]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",44.49,29.63,29.66,29.63,44.79,29.86,29.86,30.06,43.94,29.3,44.44,29.63,29.63,44.78,29.86,44.39,29.63,29.86,29.66,30.06,29.86,29.3,29.59]
[null,"31-100 kWh"]
[null,"         Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49,4.49]
[null,"         Cargo por energía activa Hora Punta-Primeros 30 kWh",{"$nulls":4},"ctm.S/./kW.h",59.24,39.5,39.5,39.5,59.24,39.5,39.5,39.5,59.24,39.5,59.24,39.5,39.5,59.24,39.5,59.24,39.5,39.5,39.5,39.5,39.5,39.5,39.5]
[null,"         Cargo por energía activa Fuera de Punta-Primeros 30 kWh",{"$nulls":4},"ctm.S/./kW.h",44.49,29.63,29.66,29.63,44.79,29.86,29.86,30.06,43.94,29.3,44.44,29.63,29.63,44.78,29.86,44.39,29.63,29.86,29.66,30.06,29.86,29.3,29.59]
[null,"         Cargo por energía activa Hora Punta-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995,78.989999999999995]
[null,"         Cargo por energía activa Fuera de Punta-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",59.32,59.25,59.32,59.25,59.72,59.72,59.72,60.12,58.59,58.59,59.25,59.25,59.25,59.71,59.71,59.18,59.25,59.72,59.32,60.12,59.71,58.59,59.18]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71,4.71]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86,82.86]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",62.23,62.15,62.23,62.15,62.65,62.65,62.65,63.07,61.46,61.46,62.15,62.15,62.15,62.64,62.64,62.08,62.15,62.65,62.23,63.07,62.64,61.46,62.08]
[null,"c) No Residencial"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79,12.79]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",128.54,128.4,128.54,128.4,129.05000000000001,129.05000000000001,129.05000000000001,129.47,127.45,127.45,128.4,128.4,128.4,131.44999999999999,131.44999999999999,128.74,128.4,129.05000000000001,128.54,129.47,131.44999999999999,127.45,128.74]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",62.23,62.15,62.23,62.15,62.65,62.65,62.65,63.07,61.46,61.46,62.15,62.15,62.15,62.64,62.64,62.08,62.15,62.65,62.23,63.07,62.64,61.46,62.08]
["BT8","SUMINISTROS RURALES CON CELDAS FOTOVOLTAICAS (Sierra)",{"$nulls":5},"Inversion 100% Estado",{"$nulls":5},"Inversion 100% Empresa",{"$nulls":5},"  "]
[null,"Tipo de Módulo",{"$nulls":5},"BT8-070","BT8-100","BT8-160","BT8-240","BT8-320","BT8-050-Pre","BT8-070","BT8-100","BT8-160","BT8-240","BT8-320","BT8-050-Pre"]
[null,"Cargo Fijo Equivalente por Energia Promedio",{"$nulls":4},"ctm.S/./kW.h",95.63,82.6,59.17,51.62,80.5,123.82,156.16,133.69999999999999,96.69,86.04,134.91,163.84]

{"sheet":"CONEXION","index":1,"n_rows":131,"n_cols":11,"rows_kept":131,"cut":false,"hidden":false,"merged":[[0,0,0,10],[129,1,129,7],[109,3,109,4],[113,2,113,4],[115,0,115,1],[116,5,116,7],[128,1,128,7],[122,1,122,4],[114,0,114,1],[14,0,26,0],[36,3,36,4],[36,5,36,6],[40,3,40,4],[62,3,62,4],[67,5,67,6],[75,3,75,4],[75,5,75,6],[68,5,68,6],[115,5,115,7],[108,3,108,4],[112,5,112,7],[119,1,119,4],[110,5,110,7],[107,5,107,7],[109,5,109,7],[87,0,87,1],[87,3,87,4],[93,3,93,4],[92,3,92,4],[78,0,78,4],[4,5,4,6],[3,5,3,6],[32,5,32,6],[51,5,51,6],[49,5,49,6],[14,5,14,6],[22,5,22,6],[23,5,23,6],[9,5,9,6],[50,3,50,4],[50,5,50,6],[42,5,42,6],[92,5,92,7],[66,5,66,6],[24,3,24,4],[41,5,41,6],[24,5,24,6],[49,3,49,4],[87,5,87,7],[6,5,6,6],[10,5,10,6],[34,5,34,6],[43,5,43,6],[3,3,3,4],[11,5,11,6],[12,5,12,6],[25,3,25,4],[25,5,25,6],[31,3,31,4],[5,5,5,6],[8,5,8,6],[35,5,35,6],[17,5,17,6],[18,5,18,6],[51,3,51,4],[63,5,63,6],[53,3,53,4],[53,5,53,6],[88,5,88,7],[89,5,89,7],[90,5,90,7],[93,5,93,7],[95,5,95,7],[7,5,7,6],[52,3,52,4],[52,5,52,6],[57,3,57,4],[57,5,57,6],[58,3,58,4],[58,5,58,6],[62,5,62,6],[65,5,65,6],[19,5,19,6],[20,5,20,6],[21,5,21,6],[47,5,47,6],[64,5,64,6],[48,5,48,6],[44,5,44,6],[45,5,45,6],[46,5,46,6],[40,5,40,6],[97,5,97,7],[96,5,96,7],[108,5,108,7],[91,5,91,7],[94,5,94,7],[105,3,105,4],[100,5,100,7],[104,3,104,4],[104,5,104,7],[101,3,101,4],[100,3,100,4],[99,5,99,7],[102,3,102,4],[103,3,103,4],[101,5,101,7],[102,5,102,7],[103,5,103,7],[1,0,1,8],[4,0,13,0],[4,1,13,1],[4,2,9,2],[4,3,4,4],[36,1,37,1],[37,3,37,4],[37,5,37,6],[34,2,35,2],[34,3,34,4],[32,0,35,0],[32,1,35,1],[32,2,33,2],[32,3,32,4],[13,5,13,6],[15,5,15,6],[33,5,33,6],[31,5,31,6],[16,5,16,6],[26,3,26,4],[26,5,26,6],[14,1,21,1],[14,2,17,2],[14,3,14,4],[10,2,13,2],[10,3,10,4],[22,3,22,4],[41,2,44,2],[41,3,41,4],[36,0,37,0],[23,3,23,4],[23,1,26,1],[18,2,21,2],[18,3,18,4],[78,9,78,10],[76,3,76,4],[76,5,76,6],[67,3,67,4],[63,3,63,4],[58,0,59,0],[58,1,59,1],[59,3,59,4],[59,5,59,6],[74,3,74,4],[74,5,74,6],[78,5,78,6],[78,7,78,8],[130,1,130,7],[124,1,124,4],[116,0,116,1],[117,5,117,7],[114,2,114,4],[110,3,110,4],[104,0,104,1],[102,0,102,1],[97,3,97,4],[127,1,127,7],[121,1,121,4],[114,5,114,7],[113,0,113,1],[126,1,126,7],[120,1,120,4],[123,1,123,4],[107,3,107,4],[106,3,106,4],[106,5,106,7],[113,5,113,7],[111,5,111,7],[111,0,111,1],[105,5,105,7],[98,5,98,7],[45,2,48,2],[45,3,45,4],[41,0,53,0],[41,1,48,1],[94,0,94,1],[94,3,94,4],[90,3,90,4],[88,0,88,1],[88,3,88,4],[50,1,53,1]]}
[]
["PRESUPUESTOS DE LA CONEXIÓN ELECTRICA (NO INCLUYE IGV)"]
["Conexiones en Baja Tensión 220 V - Soles",{"$nulls":5},"Vigente a partir del 04-06-2022"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Aérea (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT5A",null,1094,1227]
[{"$nulls":5},"BT5B (2 hilos)",null,318,448]
[{"$nulls":5},"BT5B (2 hilos) - Rural (1)",null,366]
[{"$nulls":5},"BT5B (3 hilos)",null,325,457]
[{"$nulls":5},"BT5B (3 hilos) - Rural (1)",null,373]
[{"$nulls":5},"BT6",null,235,381]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT5A",null,1123,1234]
[{"$nulls":5},"BT5B (2 hilos)",null,348,457]
[{"$nulls":5},"BT5B (3 hilos)",null,354,464]
[{"$nulls":5},"BT6",null,264,386]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5A",null,2083,2212]
[{"$nulls":5},"BT5B",null,602,732]
[{"$nulls":5},"BT6",null,411,498]
[{"$nulls":5},"BT2/BT3/BT4",null,2612,2699]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5A",null,2113,2222]
[{"$nulls":5},"BT5B",null,632,742]
[{"$nulls":5},"BT6",null,441,509]
[{"$nulls":5},"BT2/BT3/BT4",null,2779,2846]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW",null,"BT5A/BT5B/BT2/BT3/BT4",null,3565,3869]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW",null,"BT2/BT3/BT4",null,3813,4634]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW",null,"BT2/BT3/BT4",null,null,6496]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW",null,"BT2/BT3/BT4",null,null,8562]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW",null,"BT2/BT3/BT4",null,null,9384]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.            (3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
[]
["Conexiones en Baja Tensión Múltiples 220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Conexión","Caja toma (1)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT5B (2 hilos)",null,185,81]
[{"$nulls":5},"BT5B (3 hilos)",null,191,81]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT5B (2 hilos)",null,201,144]
[{"$nulls":5},"BT5B (3 hilos)",null,208,144]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5B",null,386,146]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5B",null,412,298]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["Conexiones en Baja Tensión 380/220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                       Tarifaria",null,"Aérea            (1)","Subterránea (1)(2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5A",null,2130,2306]
[{"$nulls":5},"BT5B",null,608,785]
[{"$nulls":5},"BT6",null,418,547]
[{"$nulls":5},"BT2/BT3/BT4",null,2611,2740]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5A",null,2134,2311]
[{"$nulls":5},"BT5B",null,611,788]
[{"$nulls":5},"BT6",null,421,551]
[{"$nulls":5},"BT2/BT3/BT4",null,2615,2745]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW",null,"BT5A/BT5B/BT2/BT3/BT4",null,3366,3700]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW",null,"BT2/BT3/BT4",null,3606,4066]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW",null,"BT2/BT3/BT4",null,null,5243]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW",null,"BT2/BT3/BT4",null,null,7337]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW",null,"BT2/BT3/BT4",null,null,8040]
["(1) Aplicable a conexiones con acometida simple o doble."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 380/220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Conexión","Caja Toma (1)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5B",null,384,121]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5B",null,388,269]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["Conexiones en Baja Tensión 220 V - Prepago - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Aérea            (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT7 (2 hilos)",null,690,823]
[{"$nulls":5},"BT7 (2 hilos) - Rural (1)",null,738]
[{"$nulls":5},"BT7 (3 hilos)",null,960,828]
[{"$nulls":5},"BT7 (3 hilos) - Rural (1)",null,1008]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT7 (2 hilos)",null,719,829]
[{"$nulls":5},"BT7 (3 hilos)",null,991,844]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble."]
["(3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
[]
["Costo por Metro de Cable de Conexiones en Baja Tensión 220 V - Prepago - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Costo"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT7",null,5]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT7",null,7]
[]
["Conexiones Básicas en Media Tensión - Soles",{"$nulls":4},"10 kV",null,"13.2/7.62 kV",null,"20 kV - 22.9/13.2 kV"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","PMI","Celda","PMI","Celda","PMI","Celda"]
["Trifásica","C5","C5.1","Pc ≤ 100 kW","MT2/MT3/MT4",11135,19031,13660,24861,15361,24897]
[null,null,"C5.2","100 kW < Pc ≤ 400 kW","MT2/MT3/MT4",14892,17121,13742,22322,15361,24897]
[null,null,"C5.3","400 kW < Pc ≤ 700 kW","MT2/MT3/MT4",13373,16368,14125,21321,16113,27864]
[null,null,"C5.4","700 kW < Pc ≤ 1000 kW","MT2/MT3/MT4",13811,15548,14125,21321,16469,27183]
[null,null,"C5.5","1000 kW < Pc ≤ 2500 kW","MT2/MT3/MT4",16865,16260,15402,20989,18064,25292]
[]
["Otros Elementos Electromecánicos en Media Tensión - Soles"]
["Elemento",null,"Tipo de red","Potencia Conectada (Pc)",null,"Descripción",null,null,"10 kV","13.2/7.62 kV","20 kV - 22.9/13.2 kV"]
["Empalme de acometida",null,"Aérea","Pc ≤ 1000 kW",null,"A red aérea con cable autoportante",null,null,1296,1123,1074]
[{"$nulls":5},"A red aérea con conductor desnudo",null,null,199,199,199]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"A red aérea con cable autoportante",null,null,1296,1123,1074]
[{"$nulls":5},"A red aérea con conductor desnudo",null,null,199,199,199]
[null,null,"Subterránea","Pc ≤ 1000 kW",null,"A red subterránea",null,null,7342,7342,7342]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"A red subterránea",null,null,7342,7342,7342]
["Cable de acometida",null,"Aérea","Pc ≤ 1000 kW",null,"Con cable autoportante y salida a red subterránea",null,null,7682,7337,7449]
[{"$nulls":5},"Con conductor desnudo y salida a red aérea",null,null,6247,6260,6595]
[{"$nulls":5},"Con conductor desnudo y salida a red subterránea",null,null,6393,6233,6272]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con cable autoportante y salida a red subterránea",null,null,8104,7337,7449]
[{"$nulls":5},"Con conductor desnudo y salida a red aérea",null,null,7204,6314,6595]
[{"$nulls":5},"Con conductor desnudo y salida a red subterránea",null,null,7052,6288,6272]
[null,null,"Subterránea-Aérea","Pc ≤ 1000 kW",null,"Con conductor desnudo y salida a red subterránea",null,null,7416,7070,7863]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con conductor desnudo y salida a red subterránea",null,null,8013,7070,7863]
["Caja de protección",null,"Subterránea","Pc ≤ 1000 kW",null,"Para celda interior",null,null,7191,6925,7163]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Para celda interior",null,null,7191,6925,7163]
["Sistema de protección y seccionamiento",null,"Aérea","Pc ≤ 100 kW",null,"Con seccionador cut-out",null,null,1727,1617,1819]
[null,null,null,"100 kW < Pc ≤ 400 kW",null,"Con seccionador cut-out",null,null,1732,1612,1820]
[null,null,null,"400 kW < Pc ≤ 700 kW",null,"Con seccionador cut-out",null,null,1754,1631,1820]
[null,null,null,"700 kW < Pc ≤ 1000 kW",null,"Con seccionador cut-out",null,null,1792,1648,1824]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con seccionador cut-out",null,null,7483,6667,7161]
[null,null,"Subterránea","Pc ≤ 1000 kW",null,"Con seccionador de potencia para celda interior",null,null,19676,20605,26420]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con seccionador de potencia para celda interior",null,null,31567,32602,26281]
["Protección sobretensión",null,"Aérea",null,null,"Para instalación exterior",null,null,1042,1110,1402]
[null,null,"Subterránea",null,null,"Para instalación interior",null,null,1658,2007,2266]
["Zanja (metro lineal)",null,"Aérea/Subterránea",null,null,"Para PMI o celda interior",null,null,64,64,64]
["Rotura y reparación de vereda (m2)",null,"Aérea/Subterránea",null,null,"Para PMI o celda interior",null,null,156,156,156]
["Murete",null,"Aérea",null,null,"Para PMI",null,null,334,334,334]
["Protección de estructuras",null,"Aérea",null,null,"Bloque de concreto",null,null,569,569,569]
[{"$nulls":5},"Riel de acero",null,null,185,185,185]
[null,"Costo por Vereda, Murete y Mástil en Baja Tensión - Soles"]
[null,"Descripción",null,null,null,"Unidad","Costo"]
[null,"Rotura y resane de vereda en baja tensión",null,null,null,"m2",156]
[null,"Murete baja tensión, conexión monofásica",null,null,null,"Unidad",192]
[null,"Murete baja tensión, conexión trifásica",null,null,null,"Unidad",213]
[null,"Mástil metálico de 3 m",null,null,null,"Unidad",97]
[null,"Mástil metálico de 6 m",null,null,null,"Unidad",152]
[null,"Costos Adicionales al Sistema de Proteccion y Seccionamiento - Soles"]
[null,"Descripción",{"$nulls":6},"Unidad","Costo"]
[null,"Seccionador Tipo Expulsión, Exterior, Unipolar, Bajo Carga, 10kV, 300A x 3 (1)",{"$nulls":6},"Unidad",2247]
[null,"Seccionador Tipo Expulsión, Exterior, Unipolar, Bajo Carga, 22.9kV, 200A x 3 (1)",{"$nulls":6},"Unidad",3726]
[null,"Seccionador Bajo Carga, Interior, Tripolar, 10kV, 400A x 1 (2)",{"$nulls":6},"Unidad",6140]
[null,"Aislador Extensor, Polimerico, 25kv, Para Cut-Out x 3 (3)",{"$nulls":6},"Unidad",861]

{"sheet":"REP_MTTO","index":2,"n_rows":95,"n_cols":15,"rows_kept":95,"cut":false,"hidden":false,"merged":[[3,11,3,12],[3,13,3,14],[1,0,1,14],[15,0,28,0],[15,1,22,1],[15,2,18,2],[11,2,14,2],[11,3,14,3],[25,1,28,1],[19,2,22,2],[19,3,22,3],[15,3,18,3],[5,0,14,0],[5,1,14,1],[5,2,10,2],[5,3,10,3],[3,7,3,8],[3,9,3,10],[32,0,32,4],[32,5,32,6],[32,7,32,8],[32,9,32,10],[32,11,32,12],[54,8,54,14],[43,7,43,8],[43,9,43,10],[43,11,43,12],[43,13,43,14],[62,5,62,6],[62,7,62,8],[62,9,62,10],[62,11,62,12],[81,0,85,0],[81,1,85,1],[70,1,75,1],[70,2,73,2],[74,2,75,2],[79,0,79,4],[79,5,79,6],[79,7,79,8],[79,9,79,10]]}
[]
["CARGOS DE REPOSICION Y MANTENIMIENTO  DE LA CONEXIÓN ELECTRICA (NO INCLUYE IGV)"]
["Conexiones en Baja Tensión 220 V - Nuevos Soles",{"$nulls":6},"Vigente a partir del 04-06-2022"]
[{"$nulls":7},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT5A",1.75,1.77]
[{"$nulls":4},"BT5B (2 hilos)",null,null,1.27,1.29,1.33,1.35,1.52,1.54,1.58,1.6]
[{"$nulls":4},"BT5B (2 hilos) - Rural (1)",null,null,1.48,null,1.55,null,1.79,null,1.8599999999999999]
[{"$nulls":4},"BT5B (3 hilos)",null,null,1.27,1.29,1.33,1.35,1.52,1.54,1.58,1.6]
[{"$nulls":4},"BT5B (3 hilos) - Rural (1)",null,null,1.53,null,1.6,null,1.84,null,1.91]
[{"$nulls":4},"BT6",0.74,0.75]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT5A",1.7999999999999998,1.77]
[{"$nulls":4},"BT5B (2 hilos)",null,null,1.27,1.29,1.33,1.35,1.52,1.54,1.58,1.6]
[{"$nulls":4},"BT5B (3 hilos)",null,null,1.27,1.29,1.33,1.35,1.52,1.54,1.58,1.6]
[{"$nulls":4},"BT6",0.74,0.75]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5A",3.32,3.37]
[{"$nulls":4},"BT5B",null,null,1.76,1.8199999999999998,1.76,1.8199999999999998,1.9,1.9500000000000002,1.9,1.9500000000000002]
[{"$nulls":4},"BT6",0.81,0.80999999999999994]
[{"$nulls":4},"BT2/BT3/BT4",3.8699999999999997,3.93]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5A",3.32,3.37]
[{"$nulls":4},"BT5B",null,null,1.76,1.8199999999999998,1.76,1.8199999999999998,1.9,1.9500000000000002,1.9,1.9500000000000002]
[{"$nulls":4},"BT6",0.81,0.80999999999999994]
[{"$nulls":4},"BT2/BT3/BT4",3.92,3.97]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW","BT5B",5.35,5.3000000000000007]
[{"$nulls":4},"BT5A/BT2/BT3/BT4",5.35,5.3000000000000007]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW","BT2/BT3/BT4",5.42,5.5500000000000007]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW","BT2/BT3/BT4",null,6.16]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW","BT2/BT3/BT4",null,6.84]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW","BT2/BT3/BT4",null,7.08]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.            (3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 220 V - Nuevos Soles"]
[{"$nulls":5},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT5B (2 hilos)",1.32,1.22,1.3800000000000001,1.28,1.57,1.47,1.6300000000000001,1.53]
[{"$nulls":4},"BT5B (3 hilos)",1.35,1.25,1.4100000000000001,1.31,1.6,1.5,1.6600000000000001,1.56]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT5B (2 hilos)",1.35,1.25,1.4100000000000001,1.31,1.6,1.5,1.6600000000000001,1.56]
[{"$nulls":4},"BT5B (3 hilos)",1.35,1.25,1.4100000000000001,1.31,1.6,1.5,1.6600000000000001,1.56]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5B",1.8,1.74,1.8,1.74,1.94,1.87,1.94,1.87]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5B",1.8399999999999999,1.7799999999999998,1.8399999999999999,1.7799999999999998,1.98,1.9100000000000001,1.98,1.9100000000000001]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión 380/220 V - Nuevos Soles"]
[{"$nulls":7},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5A",3.32,3.37]
[{"$nulls":4},"BT5B",null,null,1.76,1.85,1.76,1.85,1.9,1.98,1.9,1.98]
[{"$nulls":4},"BT6",0.81,0.86]
[{"$nulls":4},"BT2/BT3/BT4",3.8699999999999997,3.93]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5A",3.32,3.37]
[{"$nulls":4},"BT5B",null,null,1.76,1.85,1.76,1.85,1.9,1.98,1.9,1.98]
[{"$nulls":4},"BT6",0.81,0.86]
[{"$nulls":4},"BT2/BT3/BT4",3.8699999999999997,3.93]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW","BT5B",5.3,5.2200000000000006]
[{"$nulls":4},"BT5A/BT2/BT3/BT4",5.3,5.2200000000000006]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW","BT2/BT3/BT4",5.38,5.34]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW","BT2/BT3/BT4",null,5.76]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW","BT2/BT3/BT4",null,6.42]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW","BT2/BT3/BT4",null,6.67]
["(1) Aplicable a conexiones con acometida simple o doble."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 380/220 V - Nuevos Soles"]
[{"$nulls":5},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5B",1.8,1.74,1.8,1.74,1.94,1.87,1.94,1.87]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5B",1.8399999999999999,1.7799999999999998,1.8399999999999999,1.7799999999999998,1.98,1.9100000000000001,1.98,1.9100000000000001]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión 220 V - Prepago - Nuevos Soles"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea              (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT7 (2 hilos)",1.83,1.85]
[{"$nulls":4},"BT7 (2 hilos) - Rural (1)",1.83,0.74]
[{"$nulls":4},"BT7 (3 hilos)",2.39,2.31]
[{"$nulls":4},"BT7 (3 hilos) - Rural (1)",2.42,0.74]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT7 (2 hilos)",1.83,1.85]
[{"$nulls":4},"BT7 (3 hilos)",2.39,2.31]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.",null,null,null,"(3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Media Tensión - Nuevos Soles"]
[{"$nulls":5},"10 kV",null,"13.2/7.62 kV",null,"20 kV - 22.9/13.2 kV"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","PMI","Celda","PMI","Celda","PMI","Celda"]
["Trifásica","C5","C5.1","Pc ≤ 100 kW","MT2/MT3/MT4",18.86,26.93,19.61,29.12,20.880000000000003,31.83]
[null,null,"C5.2","100 kW < Pc ≤ 400 kW","MT2/MT3/MT4",20.100000000000001,26.3,19.649999999999999,28.3,20.880000000000003,31.83]
[null,null,"C5.3","400 kW < Pc ≤ 700 kW","MT2/MT3/MT4",19.61,26.060000000000002,19.759999999999998,28,21.15,32.799999999999997]
[null,null,"C5.4","700 kW < Pc ≤ 1000 kW","MT2/MT3/MT4",19.72,25.810000000000002,19.759999999999998,28,21.259999999999998,32.57]
[null,null,"C5.5","1000 kW < Pc ≤ 2500 kW","MT2/MT3/MT4",21.310000000000002,26.880000000000003,20.740000000000002,28.73,22.6,32.549999999999997]
{"$rows_empty":8}
["  "]

{"sheet":"COR_RECONEX","index":3,"n_rows":113,"n_cols":6,"rows_kept":113,"cut":false,"hidden":false,"merged":[[111,0,111,1],[112,0,112,1],[84,0,95,0],[98,0,98,3],[98,4,98,5],[100,0,107,0],[110,0,110,1],[64,0,64,3],[64,4,64,5],[66,0,79,0],[82,0,82,3],[82,4,82,5],[45,4,45,5],[47,0,52,0],[50,1,52,1],[54,0,54,3],[54,4,54,5],[15,4,15,5],[17,0,22,0],[20,1,22,1],[17,1,19,1],[0,0,0,5],[1,0,1,5],[4,0,4,2],[4,3,5,3],[6,0,13,0],[6,1,9,1],[10,1,13,1],[56,0,61,0],[58,1,59,1],[60,1,61,1],[24,0,24,3],[26,0,31,0],[28,1,29,1],[47,1,49,1],[45,0,45,3],[30,1,31,1],[34,0,34,2],[34,3,35,3],[36,0,43,0],[36,1,39,1],[40,1,43,1]]}
[]
["IMPORTES MAXIMOS DE CORTE Y RECONEXION (NO INCLUYE IGV)"]
["Conexiones monofásicas, hasta 10 kW, BT5A, BT5B y BT6"]
[null,null,"Vigente a partir del 04-06-2022"]
["Descripción",null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Fusible o interruptor (tapa sin ranura)",7.59]
[null,null,"Interruptor (tapa con ranura)",10.29]
[null,null,"Caja de medición (aislamiento acometida)",11.04]
[null,null,"Línea aérea (empalme)",26.41]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)",9.15]
[null,null,"Interruptor (tapa con ranura)",11.82]
[null,null,"Caja de medición (aislamiento acometida)",12.68]
[null,null,"Línea aérea (empalme)",32.08]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Retiro","RT conexión aérea","Camioneta",53.04,56.88]
[null,null,"RT conexión subterránea","Camioneta",54.02,57.65]
[null,null,"RT conexión mixta","Camioneta",54.02,57.65]
[null,"Reinstalación","RIconexión aérea","Camioneta",93.77,101]
[null,null,"RI conexión subterránea","Camioneta",70.42,76.150000000000006]
[null,null,"RI conexión mixta","Camioneta",70.42,76.150000000000006]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Caja de medición (aislamiento acometida bloqueada)","Camioneta",24.37,28.46]
[null,"Reconexión","Caja de medición (aislamiento acometida bloqueada)","Camioneta",22,27.04]
[null,"Retiro","RT conexión subterránea (empalme y cable de acometida)","Camioneta",180.91,188.15]
[null,null,"RT conexión mixta (empalme y cable de acometida)","Camioneta",180.91,188.15]
[null,"Reinstalación","RI conexión subterránea (empalme y cable de acometida)","Camioneta",249.6,259.26]
[null,null,"RI conexión mixta (empalme y cable de acometida)","Camioneta",249.6,259.26]
[]
["Conexiones Trifásicas, hasta 20 kW, BT5A, BT5B y BT6"]
["Descripción",null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Fusible o interruptor (tapa sin ranura)",9.02]
[null,null,"Interruptor (tapa con ranura)",11.46]
[null,null,"Caja de medición (aislamiento acometida)",11.57]
[null,null,"Línea aérea (empalme)",26.14]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)",12.11]
[null,null,"Interruptor (tapa con ranura)",14.12]
[null,null,"Caja de medición (aislamiento acometida)",15.13]
[null,null,"Línea aérea (empalme)",32.99]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Retiro","RT conexión aérea","Camioneta",63.1,67.930000000000007]
[null,null,"RT conexión subterránea","Camioneta",58.63,62.24]
[null,null,"RT conexión mixta","Camioneta",58.63,62.24]
[null,"Reinstalación","RI conexión aérea","Camioneta",108.2,116.46]
[null,null,"RI conexión subterránea","Camioneta",79,85.43]
[null,null,"RI conexión mixta","Camioneta",79,85.43]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Caja de medición (aislamiento acometida bloqueada)","Camioneta",27.64,32.47]
[null,"Reconexión","Caja de medición (aislamiento acometida bloqueada)","Camioneta",29.77,33.53]
[null,"Retiro","RT conexión subterránea (empalme y cable de acometida)","Camioneta",198.53,205.77]
[null,null,"RT conexión mixta (empalme y cable de acometida)","Camioneta",198.53,205.77]
[null,"Reinstalación","RI conexión subterránea (empalme y cable de acometida)","Camioneta",291.49,291.49]
[null,null,"RI conexión mixta (empalme y cable de acometida)","Camioneta",281.87,290.33999999999997]
[]
["Conexiones Trifásicas, hasta 20 kW, resto de opciones (BT2,BT3 y BT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW resto de opciones (BT2,BT3 y BT4)","Corte","Fusible o interruptor (tapa sin ranura)","Camioneta",25.47,27.52]
[null,null,"Interruptor (tapa con ranura)","Camioneta",28.5,30.84]
[null,null,"Caja de medición (aislamiento acometida)","Camioneta",28.67,30.96]
[null,null,"Línea aérea (empalme)","Camioneta",40.81,43.71]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)","Camioneta",41.39,43.63]
[null,null,"Interruptor (tapa con ranura)","Camioneta",32.229999999999997,34.880000000000003]
[null,null,"Caja de medición (aislamiento acometida)","Camioneta",45.23,47.27]
[null,null,"Línea aérea (empalme)","Camioneta",61.26,64.290000000000006]
[null,"Retiro","RT conexión aérea","Camioneta",63.1,67.930000000000007]
[null,null,"RT conexión subterránea","Camioneta",58.63,62.24]
[null,null,"RT conexión mixta","Camioneta",58.63,62.24]
[null,"Reinstalación","RIconexión aérea","Camioneta",120.55,128.81]
[null,null,"RIión subterránea","Camioneta",91.36,97.82]
[null,null,"RI conexión mixta","Camioneta",91.36,97.82]
[]
["Conexiones trifásicas mayor a 20 kW, resto de opciones (BT2,BT3 y BT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica mayor a 20 kW resto de opciones (BT2,BT3 y BT4)","Corte","En fusible o interruptor (tapa sin ranura)","Camioneta",28.42,30.71]
[null,null,"En caja de medición (aislamiento acometida)","Camioneta",31.08,33.57]
[null,null,"En línea aérea (empalme)","Camioneta",46.17,49.28]
[null,"Reconexión","En fusible o interruptor (tapa sin ranura)","Camioneta",37.25,39.54]
[null,null,"En caja de medición (aislamiento acometida)","Camioneta",46.62,49.64]
[null,null,"En línea aérea (empalme)","Camioneta",74.63,78.760000000000005]
[null,"Retiro","En conexión aérea","Camioneta",92.01,99.2]
[null,null,"En conexión subterránea","Camioneta",86.17,92.58]
[null,null,"En conexión mixta","Camioneta",86.17,92.58]
[null,"Reinstalación","En conexión aérea","Camioneta",137.6,147.21]
[null,null,"En conexión subterránea","Camioneta",110.94,119.2]
[null,null,"En conexión mixta","Camioneta",110.94,119.2]
[]
["Conexiones trifásicas, hasta 2500 kW, resto de opciones (MT2,MT3 y MT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 2500 kW resto de opciones (MT2,MT3 y MT4)","Corte","En sistema de protección - PMI","Camioneta",57.91,62.72]
[null,null,"En sistema de protección - Celda","Camioneta",57.86,62.65]
[null,"Reconexión","En sistema de protección - PMI","Camioneta",57.86,62.65]
[null,null,"En sistema de protección - Celda","Camioneta",69.44,75.17]
[null,"Retiro","En sistema de protección - PMI","Camioneta",244.09,253.69]
[null,null,"En sistema de protección - Celda","Camioneta",99.13,107.38]
[null,"Reinstalación","En sistema de protección - PMI","Camioneta",432.03,443.6]
[null,null,"En sistema de protección - Celda","Camioneta",254.76,264.42]
[]
["Suministros Rurales con Celdas Fotovoltaicas (Sierra)"]
["Tipo",null,"Costo Total (S/.)"]
["Corte",null,8.27]
["Reconexión",null,10.37]