{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["ENERGIA","CONEXION","REP_MTTO","COR_RECONEX"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ENERGIA","index":0,"n_rows":149,"n_cols":30,"rows_kept":149,"cut":false,"hidden":false,"merged":[[0,7,0,29],[1,0,1,1],[2,0,2,5],[146,7,146,12],[146,13,146,18]]}
["PLIEGO TARIFARIO DEL SERVICIO PUBLICO DE ELECTRICIDAD (NO INCLUYE IGV)"]
["2022-05-01",{"$nulls":14},"VIGENTE A PARTIR DEL DIA 01-05-2022-R"]
["SISTEMA ELECTRICO",{"$nulls":6},"Cusco","Valle Sagrado 1","Valle Sagrado 2","Valle Sagrado 3","Sicuani","Sicuani Rural","Combapata, Chumbivilcas","Yauri","La Convención, Macupicchu","La Convención Rural","Abancay","Abancay Rural, Chuquibambilla, Chacapuente","Andahuyalas","Puerto Maldonado","Puerto Maldonad Rural-Iñapari-Iberia","Mazuko","SER-Apurimac y Valle Sagrado","SER-Valle Vilcanota","SER-Quispicanchis","SER-Espinar","SER-Iberia","SER-Machupicchu","SER-Mazuko"]
["MEDIA TENSION",{"$nulls":5},"UNIDAD",{"$nulls":10},"TARIFA"]
["MT2","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",33.340000000000003,33.200000000000003,33.340000000000003,33.200000000000003,33.799999999999997,33.799999999999997,33.799999999999997,34.19,32.340000000000003,32.340000000000003,33.200000000000003,33.200000000000003,33.200000000000003,36.01,36.01,33.53,33.200000000000003,33.799999999999997,33.340000000000003,34.19,36.01,32.340000000000003,33.53]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",27.87,27.8,27.87,27.8,28.26,28.26,28.26,28.65,27.17,27.17,27.8,27.8,27.8,28.25,28.25,27.74,27.8,28.26,27.87,28.65,28.25,27.17,27.74]
[null,"Cargo por Potencia Activa de Generación en HP",{"$nulls":4},"S/./kW-mes",65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17,65.17]
[null,"Cargo por Potencia Activa por uso de redes de Distribución en HP",{"$nulls":4},"S/./kW-mes",21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55,21.55]
[null,"Cargo por Exceso de Potencia Activa por uso de redes de Distribución en HFP",{"$nulls":4},"S/./kW-mes",22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05,22.05]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83]
["MT3","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",33.340000000000003,33.200000000000003,33.340000000000003,33.200000000000003,33.799999999999997,33.799999999999997,33.799999999999997,34.19,32.340000000000003,32.340000000000003,33.200000000000003,33.200000000000003,33.200000000000003,36.01,36.01,33.53,33.200000000000003,33.799999999999997,33.340000000000003,34.19,36.01,32.340000000000003,33.53]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",27.87,27.8,27.87,27.8,28.26,28.26,28.26,28.65,27.17,27.17,27.8,27.8,27.8,28.25,28.25,27.74,27.8,28.26,27.87,28.65,28.25,27.17,27.74]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83]
["MT4","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41]
[null,"Cargo por Energía Activa",{"$nulls":4},"ctm.S/./kW.h",29.2,29.12,29.2,29.12,29.61,29.61,29.61,30,28.44,28.44,29.12,29.12,29.12,30.15,30.15,29.15,29.12,29.61,29.2,30,30.15,28.44,29.15]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5,59.5]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99,37.99]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07,23.07]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68,22.68]
[null,"Cargo por Energía Reactiva que Exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83]
["BAJA TENSION"]
["BT2","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54,13.54]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",36.17,36.020000000000003,36.17,36.020000000000003,36.68,36.68,36.68,37.1,35.090000000000003,35.090000000000003,36.020000000000003,36.020000000000003,36.020000000000003,39.08,39.08,36.380000000000003,36.020000000000003,36.68,36.17,37.1,39.08,35.090000000000003,36.380000000000003]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",30.24,30.17,30.24,30.17,30.66,30.66,30.66,31.08,29.48,29.48,30.17,30.17,30.17,30.65,30.65,30.1,30.17,30.66,30.24,31.08,30.65,29.48,30.1]
[null,"Cargo por Potencia Activa de Generación en HP",{"$nulls":4},"S/./kW-mes",67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007,67.430000000000007]
[null,"Cargo por Potencia Activa por uso de redes de Distribución en HP",{"$nulls":4},"S/./kW-mes",100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14,100.14]
[null,"Cargo por Exceso de Potencia Activa por uso de redes de Distribución en HFP",{"$nulls":4},"S/./kW-mes",73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007,73.680000000000007]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83]
["BT3","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",36.17,36.020000000000003,36.17,36.020000000000003,36.68,36.68,36.68,37.1,35.090000000000003,35.090000000000003,36.020000000000003,36.020000000000003,36.020000000000003,39.08,39.08,36.380000000000003,36.020000000000003,36.68,36.17,37.1,39.08,35.090000000000003,36.380000000000003]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",30.24,30.17,30.24,30.17,30.66,30.66,30.66,31.08,29.48,29.48,30.17,30.17,30.17,30.65,30.65,30.1,30.17,30.66,30.24,31.08,30.65,29.48,30.1]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83]
["BT4","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41]
[null,"Cargo por Energía Activa",{"$nulls":4},"ctm.S/./kW.h",31.69,31.61,31.69,31.61,32.14,32.14,32.14,32.56,30.85,30.85,31.61,31.61,31.61,32.72,32.72,31.64,31.61,32.14,31.69,32.56,32.72,30.85,31.64]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51,47.51]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73,45.73]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27,97.27]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56,94.56]
[null,"Cargo por Energía Reactiva que Exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83,4.83]
["BT5A","a) Usuarios con demanda maximia mensuakl de hasta 20KW en HP y HFP"]
[null,"Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",222.76,222.62,222.76,222.62,223.27,223.27,223.27,223.69,221.67,221.67,222.62,222.62,222.62,225.66,225.66,222.96,222.62,223.27,222.76,223.69,225.66,221.67,222.96]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",30.24,30.17,30.24,30.17,30.66,30.66,30.66,31.08,29.48,29.48,30.17,30.17,30.17,30.65,30.65,30.1,30.17,30.66,30.24,31.08,30.65,29.48,30.1]
[null,"Cargo por Exceso de Potencia en HFP",{"$nulls":4},"S/.kW-mes",91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02]
[null,"b) Usuarios con demanda maximia mensuakl de hasta 20KW en HP y 50KW en HFP"]
[null,"Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",263.98,263.83,263.98,263.83,264.48,264.48,264.48,264.91000000000003,262.89999999999998,262.89999999999998,263.83,263.83,263.83,266.89,266.89,264.19,263.83,264.48,263.98,264.91000000000003,266.89,262.89999999999998,264.19]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",30.24,30.17,30.24,30.17,30.66,30.66,30.66,31.08,29.48,29.48,30.17,30.17,30.17,30.65,30.65,30.1,30.17,30.66,30.24,31.08,30.65,29.48,30.1]
[null,"Cargo por Exceso de Potencia en HFP",{"$nulls":4},"S/.kW-mes",91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02,91.02]
["BT5B","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18]
[null,"           Cargo por energía activa",null,null,"   ",null,"ctm.S/./kW.h",58.04,38.69,38.69,38.69,58.04,38.69,38.69,38.69,58.04,38.69,58.04,38.69,38.69,58.04,38.69,58.04,38.69,38.69,38.69,38.69,38.69,38.69,38.69]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",17.41,11.61,11.61,11.61,17.41,11.61,11.61,11.61,17.41,11.61,17.41,11.61,11.61,17.41,11.61,17.41,11.61,11.61,11.61,11.61,11.61,11.61,11.61]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17]
[null,"c) No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",83.52,83.44,83.52,83.44,83.96,83.96,83.96,84.39,82.68,82.68,83.44,83.44,83.44,84.55,84.55,83.47,83.44,83.96,83.52,84.39,84.55,82.68,83.47]
["BT5C-AP","           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96,4.96]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",82.09,82.01,82.09,82.01,82.51,82.51,82.51,82.92,81.290000000000006,81.290000000000006,82.01,82.01,82.01,83.07,83.07,82.04,82.01,82.51,82.09,82.92,83.07,81.290000000000006,82.04]
["BT5D","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",42.65,28.39,28.43,28.39,42.95,28.63,28.63,28.82,42.08,28.06,42.59,28.39,28.39,43.34,28.89,42.61,28.39,28.63,28.43,28.82,28.89,28.06,28.41]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18,4.18]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",12.79,8.52,8.5299999999999994,8.52,12.88,8.59,8.59,8.65,12.62,8.42,12.78,8.52,8.52,13,8.67,12.78,8.52,8.59,8.5299999999999994,8.65,8.67,8.42,8.52]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",56.86,56.78,56.86,56.78,57.26,57.26,57.26,57.64,56.11,56.11,56.78,56.78,56.78,57.78,57.78,56.81,56.78,57.26,56.86,57.64,57.78,56.11,56.81]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",59.65,59.56,59.65,59.56,60.07,60.07,60.07,60.46,58.86,58.86,59.56,59.56,59.56,60.61,60.61,59.59,59.56,60.07,59.65,60.46,60.61,58.86,59.59]
[null,"c)  No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",59.65,59.56,59.65,59.56,60.07,60.07,60.07,60.46,58.86,58.86,59.56,59.56,59.56,60.61,60.61,59.59,59.56,60.07,59.65,60.46,60.61,58.86,59.59]
["BT6","Cargo Fijo Mensual - Lectura Mensual",{"$nulls":4},"S/./mes",4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38,4.38]
[null,"Cargo por Potencia",{"$nulls":4},"cent. S/./W",31.57,31.53,31.57,31.53,31.74,31.74,31.74,31.9,31.25,31.25,31.53,31.53,31.53,31.96,31.96,31.55,31.53,31.74,31.57,31.9,31.96,31.25,31.55]
["BT7","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",58.04,38.69,38.69,38.69,58.04,38.69,38.69,38.69,58.04,38.69,58.04,38.69,38.69,58.04,38.69,58.04,38.69,38.69,38.69,38.69,38.69,38.69,38.69]
[null,"31-100 kWh"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36,3.36]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",17.41,11.61,11.61,11.61,17.41,11.61,11.61,11.61,17.41,11.61,17.41,11.61,11.61,17.41,11.61,17.41,11.61,11.61,11.61,11.61,11.61,11.61,11.61]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17]
[null,"c)  No Residencial"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52,3.52]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",82.29,82.21,82.29,82.21,82.73,82.73,82.73,83.14,81.47,81.47,82.21,82.21,82.21,83.3,83.3,82.24,82.21,82.73,82.29,83.14,83.3,81.47,82.24]
["BT5E","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",58.04,38.69,38.69,38.69,58.04,38.69,38.69,38.69,58.04,38.69,58.04,38.69,38.69,58.04,38.69,58.04,38.69,38.69,38.69,38.69,38.69,38.69,38.69]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63,2.63]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",17.41,11.61,11.61,11.61,17.41,11.61,11.61,11.61,17.41,11.61,17.41,11.61,11.61,17.41,11.61,17.41,11.61,11.61,11.61,11.61,11.61,11.61,11.61]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17]
[null,"c)  No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76,2.76]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",83.5,83.41,83.5,83.41,83.94,83.94,83.94,84.36,82.66,82.66,83.41,83.41,83.41,84.52,84.52,83.44,83.41,83.94,83.5,84.36,84.52,82.66,83.44]
["BT5F","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",58.04,38.69,38.69,38.69,58.04,38.69,38.69,38.69,58.04,38.69,58.04,38.69,38.69,58.04,38.69,58.04,38.69,38.69,38.69,38.69,38.69,38.69,38.69]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",43.77,29.15,29.18,29.15,44.07,29.38,29.38,29.58,43.22,28.82,43.72,29.15,29.15,44.06,29.38,43.67,29.15,29.38,29.18,29.58,29.38,28.82,29.11]
[null,"31-100 kWh"]
[null,"         Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32,4.32]
[null,"         Cargo por energía activa Hora Punta-Primeros 30 kWh",{"$nulls":4},"ctm.S/./kW.h",58.04,38.69,38.69,38.69,58.04,38.69,38.69,38.69,58.04,38.69,58.04,38.69,38.69,58.04,38.69,58.04,38.69,38.69,38.69,38.69,38.69,38.69,38.69]
[null,"         Cargo por energía activa Fuera de Punta-Primeros 30 kWh",{"$nulls":4},"ctm.S/./kW.h",43.77,29.15,29.18,29.15,44.07,29.38,29.38,29.58,43.22,28.82,43.72,29.15,29.15,44.06,29.38,43.67,29.15,29.38,29.18,29.58,29.38,28.82,29.11]
[null,"         Cargo por energía activa Hora Punta-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38,77.38]
[null,"         Cargo por energía activa Fuera de Punta-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",58.36,58.29,58.36,58.29,58.76,58.76,58.76,59.16,57.63,57.63,58.29,58.29,58.29,58.75,58.75,58.22,58.29,58.76,58.36,59.16,58.75,57.63,58.22]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53,4.53]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17,81.17]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",61.22,61.15,61.22,61.15,61.64,61.64,61.64,62.06,60.45,60.45,61.15,61.15,61.15,61.63,61.63,61.07,61.15,61.64,61.22,62.06,61.63,60.45,61.07]
[null,"c) No Residencial"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41,12.41]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",126.87,126.72,126.87,126.72,127.37,127.37,127.37,127.8,125.79,125.79,126.72,126.72,126.72,129.77000000000001,129.77000000000001,127.08,126.72,127.37,126.87,127.8,129.77000000000001,125.79,127.08]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",61.22,61.15,61.22,61.15,61.64,61.64,61.64,62.06,60.45,60.45,61.15,61.15,61.15,61.63,61.63,61.07,61.15,61.64,61.22,62.06,61.63,60.45,61.07]
["BT8","SUMINISTROS RURALES CON CELDAS FOTOVOLTAICAS (Sierra)",{"$nulls":5},"Inversion 100% Estado",{"$nulls":5},"Inversion 100% Empresa",{"$nulls":5},"  "]
[null,"Tipo de Módulo",{"$nulls":5},"BT8-070","BT8-100","BT8-160","BT8-240","BT8-320","BT8-050-Pre","BT8-070","BT8-100","BT8-160","BT8-240","BT8-320","BT8-050-Pre"]
[null,"Cargo Fijo Equivalente por Energia Promedio",{"$nulls":4},"ctm.S/./kW.h",93.84,81.06,58.51,51.05,79.61,121.5,153.22999999999999,131.19999999999999,95.62,85.09,133.41999999999999,160.78]

{"sheet":"CONEXION","index":1,"n_rows":131,"n_cols":11,"rows_kept":131,"cut":false,"hidden":false,"merged":[[1,0,1,8],[3,3,3,4],[3,5,3,6],[78,9,78,10],[87,0,87,1],[87,3,87,4],[87,5,87,7],[90,3,90,4],[92,3,92,4],[31,3,31,4],[31,5,31,6],[32,0,35,0],[32,1,35,1],[32,2,33,2],[34,2,35,2],[34,3,34,4],[36,0,37,0],[36,1,37,1],[36,3,36,4],[4,0,13,0],[4,1,13,1],[4,2,9,2],[10,2,13,2],[10,3,10,4],[119,1,119,4],[126,1,126,7],[45,2,48,2],[45,3,45,4],[49,3,49,4],[50,1,53,1],[57,3,57,4],[57,5,57,6],[58,0,59,0],[58,1,59,1],[94,0,94,1],[97,3,97,4],[100,3,100,4],[62,5,62,6],[59,3,59,4],[105,3,105,4],[105,5,105,7],[101,3,101,4],[92,5,92,7],[95,5,95,7],[102,0,102,1],[63,3,63,4],[63,5,63,6],[75,3,75,4],[14,0,26,0],[14,1,21,1],[14,2,17,2],[14,3,14,4],[18,2,21,2],[18,3,18,4],[22,3,22,4],[23,1,26,1],[4,3,4,4],[26,3,26,4],[4,5,4,6],[23,3,23,4],[5,5,5,6],[11,5,11,6],[6,5,6,6],[12,5,12,6],[13,5,13,6],[16,5,16,6],[25,3,25,4],[25,5,25,6],[24,3,24,4],[24,5,24,6],[20,5,20,6],[21,5,21,6],[22,5,22,6],[7,5,7,6],[8,5,8,6],[9,5,9,6],[10,5,10,6],[19,5,19,6],[14,5,14,6],[15,5,15,6],[17,5,17,6],[18,5,18,6],[26,5,26,6],[23,5,23,6],[41,0,53,0],[41,1,48,1],[41,2,44,2],[89,5,89,7],[91,5,91,7],[88,0,88,1],[88,3,88,4],[88,5,88,7],[66,5,66,6],[67,5,67,6],[68,5,68,6],[76,3,76,4],[76,5,76,6],[90,5,90,7],[67,3,67,4],[74,3,74,4],[74,5,74,6],[78,0,78,4],[78,5,78,6],[78,7,78,8],[42,5,42,6],[62,3,62,4],[75,5,75,6],[64,5,64,6],[65,5,65,6],[59,5,59,6],[104,0,104,1],[106,3,106,4],[106,5,106,7],[103,3,103,4],[103,5,103,7],[104,3,104,4],[104,5,104,7],[96,5,96,7],[93,5,93,7],[94,3,94,4],[94,5,94,7],[93,3,93,4],[100,5,100,7],[101,5,101,7],[102,3,102,4],[102,5,102,7],[97,5,97,7],[98,5,98,7],[99,5,99,7],[114,2,114,4],[111,0,111,1],[113,0,113,1],[110,3,110,4],[110,5,110,7],[107,3,107,4],[107,5,107,7],[108,3,108,4],[108,5,108,7],[113,5,113,7],[109,3,109,4],[109,5,109,7],[113,2,113,4],[36,5,36,6],[37,5,37,6],[35,5,35,6],[33,5,33,6],[40,3,40,4],[40,5,40,6],[128,1,128,7],[129,1,129,7],[130,1,130,7],[121,1,121,4],[122,1,122,4],[123,1,123,4],[124,1,124,4],[120,1,120,4],[127,1,127,7],[117,5,117,7],[114,5,114,7],[111,5,111,7],[112,5,112,7],[115,0,115,1],[115,5,115,7],[116,0,116,1],[116,5,116,7],[114,0,114,1],[0,0,0,10],[58,3,58,4],[58,5,58,6],[44,5,44,6],[45,5,45,6],[46,5,46,6],[50,5,50,6],[51,3,51,4],[51,5,51,6],[41,3,41,4],[41,5,41,6],[50,3,50,4],[52,5,52,6],[53,3,53,4],[43,5,43,6],[49,5,49,6],[52,3,52,4],[53,5,53,6],[47,5,47,6],[48,5,48,6],[32,3,32,4],[32,5,32,6],[37,3,37,4],[34,5,34,6]]}
[]
["PRESUPUESTOS DE LA CONEXIÓN ELECTRICA (NO INCLUYE IGV)"]
["Conexiones en Baja Tensión 220 V - Soles",{"$nulls":5},"Vigente a partir del 04-04-2022"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Aérea (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT5A",null,1079,1210]
[{"$nulls":5},"BT5B (2 hilos)",null,313,442]
[{"$nulls":5},"BT5B (2 hilos) - Rural (1)",null,360]
[{"$nulls":5},"BT5B (3 hilos)",null,320,451]
[{"$nulls":5},"BT5B (3 hilos) - Rural (1)",null,367]
[{"$nulls":5},"BT6",null,232,375]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT5A",null,1108,1217]
[{"$nulls":5},"BT5B (2 hilos)",null,343,451]
[{"$nulls":5},"BT5B (3 hilos)",null,349,458]
[{"$nulls":5},"BT6",null,261,381]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5A",null,2054,2181]
[{"$nulls":5},"BT5B",null,594,722]
[{"$nulls":5},"BT6",null,405,491]
[{"$nulls":5},"BT2/BT3/BT4",null,2576,2662]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5A",null,2084,2192]
[{"$nulls":5},"BT5B",null,623,731]
[{"$nulls":5},"BT6",null,435,502]
[{"$nulls":5},"BT2/BT3/BT4",null,2740,2807]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW",null,"BT5A/BT5B/BT2/BT3/BT4",null,3510,3809]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW",null,"BT2/BT3/BT4",null,3754,4562]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW",null,"BT2/BT3/BT4",null,null,6395]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW",null,"BT2/BT3/BT4",null,null,8429]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW",null,"BT2/BT3/BT4",null,null,9239]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.            (3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
[]
["Conexiones en Baja Tensión Múltiples 220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Conexión","Caja toma (1)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT5B (2 hilos)",null,183,80]
[{"$nulls":5},"BT5B (3 hilos)",null,188,80]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT5B (2 hilos)",null,199,142]
[{"$nulls":5},"BT5B (3 hilos)",null,206,142]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5B",null,381,144]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5B",null,406,294]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["Conexiones en Baja Tensión 380/220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                       Tarifaria",null,"Aérea            (1)","Subterránea (1)(2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5A",null,2101,2274]
[{"$nulls":5},"BT5B",null,599,774]
[{"$nulls":5},"BT6",null,412,540]
[{"$nulls":5},"BT2/BT3/BT4",null,2575,2703]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5A",null,2104,2279]
[{"$nulls":5},"BT5B",null,603,777]
[{"$nulls":5},"BT6",null,416,543]
[{"$nulls":5},"BT2/BT3/BT4",null,2579,2707]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW",null,"BT5A/BT5B/BT2/BT3/BT4",null,3314,3642]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW",null,"BT2/BT3/BT4",null,3551,4003]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW",null,"BT2/BT3/BT4",null,null,5162]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW",null,"BT2/BT3/BT4",null,null,7223]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW",null,"BT2/BT3/BT4",null,null,7916]
["(1) Aplicable a conexiones con acometida simple o doble."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 380/220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Conexión","Caja Toma (1)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5B",null,379,119]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5B",null,382,265]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["Conexiones en Baja Tensión 220 V - Prepago - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Aérea            (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT7 (2 hilos)",null,681,812]
[{"$nulls":5},"BT7 (2 hilos) - Rural (1)",null,728]
[{"$nulls":5},"BT7 (3 hilos)",null,947,816]
[{"$nulls":5},"BT7 (3 hilos) - Rural (1)",null,994]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT7 (2 hilos)",null,710,817]
[{"$nulls":5},"BT7 (3 hilos)",null,977,832]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble."]
["(3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
[]
["Costo por Metro de Cable de Conexiones en Baja Tensión 220 V - Prepago - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Costo"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT7",null,5]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT7",null,6]
[]
["Conexiones Básicas en Media Tensión - Soles",{"$nulls":4},"10 kV",null,"13.2/7.62 kV",null,"20 kV - 22.9/13.2 kV"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","PMI","Celda","PMI","Celda","PMI","Celda"]
["Trifásica","C5","C5.1","Pc ≤ 100 kW","MT2/MT3/MT4",11060,18903,13569,24695,15258,24730]
[null,null,"C5.2","100 kW < Pc ≤ 400 kW","MT2/MT3/MT4",14792,17006,13650,22172,15258,24730]
[null,null,"C5.3","400 kW < Pc ≤ 700 kW","MT2/MT3/MT4",13284,16259,14030,21178,16005,27677]
[null,null,"C5.4","700 kW < Pc ≤ 1000 kW","MT2/MT3/MT4",13718,15444,14030,21178,16358,27001]
[null,null,"C5.5","1000 kW < Pc ≤ 2500 kW","MT2/MT3/MT4",16752,16151,15298,20848,17943,25123]
[]
["Otros Elementos Electromecánicos en Media Tensión - Soles"]
["Elemento",null,"Tipo de red","Potencia Conectada (Pc)",null,"Descripción",null,null,"10 kV","13.2/7.62 kV","20 kV - 22.9/13.2 kV"]
["Empalme de acometida",null,"Aérea","Pc ≤ 1000 kW",null,"A red aérea con cable autoportante",null,null,1271,1101,1054]
[{"$nulls":5},"A red aérea con conductor desnudo",null,null,195,195,195]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"A red aérea con cable autoportante",null,null,1271,1101,1054]
[{"$nulls":5},"A red aérea con conductor desnudo",null,null,195,195,195]
[null,null,"Subterránea","Pc ≤ 1000 kW",null,"A red subterránea",null,null,7202,7202,7202]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"A red subterránea",null,null,7202,7202,7202]
["Cable de acometida",null,"Aérea","Pc ≤ 1000 kW",null,"Con cable autoportante y salida a red subterránea",null,null,7535,7197,7307]
[{"$nulls":5},"Con conductor desnudo y salida a red aérea",null,null,6128,6140,6469]
[{"$nulls":5},"Con conductor desnudo y salida a red subterránea",null,null,6272,6114,6153]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con cable autoportante y salida a red subterránea",null,null,7949,7197,7307]
[{"$nulls":5},"Con conductor desnudo y salida a red aérea",null,null,7067,6194,6469]
[{"$nulls":5},"Con conductor desnudo y salida a red subterránea",null,null,6918,6168,6153]
[null,null,"Subterránea-Aérea","Pc ≤ 1000 kW",null,"Con conductor desnudo y salida a red subterránea",null,null,7274,6935,7713]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con conductor desnudo y salida a red subterránea",null,null,7860,6935,7713]
["Caja de protección",null,"Subterránea","Pc ≤ 1000 kW",null,"Para celda interior",null,null,7054,6793,7027]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Para celda interior",null,null,7054,6793,7027]
["Sistema de protección y seccionamiento",null,"Aérea","Pc ≤ 100 kW",null,"Con seccionador cut-out",null,null,1694,1586,1784]
[null,null,null,"100 kW < Pc ≤ 400 kW",null,"Con seccionador cut-out",null,null,1699,1581,1785]
[null,null,null,"400 kW < Pc ≤ 700 kW",null,"Con seccionador cut-out",null,null,1720,1600,1785]
[null,null,null,"700 kW < Pc ≤ 1000 kW",null,"Con seccionador cut-out",null,null,1758,1616,1789]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con seccionador cut-out",null,null,7340,6540,7024]
[null,null,"Subterránea","Pc ≤ 1000 kW",null,"Con seccionador de potencia para celda interior",null,null,19301,20212,25916]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con seccionador de potencia para celda interior",null,null,30965,31980,25780]
["Protección sobretensión",null,"Aérea",null,null,"Para instalación exterior",null,null,1023,1089,1375]
[null,null,"Subterránea",null,null,"Para instalación interior",null,null,1626,1969,2223]
["Zanja (metro lineal)",null,"Aérea/Subterránea",null,null,"Para PMI o celda interior",null,null,62,62,62]
["Rotura y reparación de vereda (m2)",null,"Aérea/Subterránea",null,null,"Para PMI o celda interior",null,null,152,152,152]
["Murete",null,"Aérea",null,null,"Para PMI",null,null,324,324,324]
["Protección de estructuras",null,"Aérea",null,null,"Bloque de concreto",null,null,552,552,552]
[{"$nulls":5},"Riel de acero",null,null,180,180,180]
[null,"Costo por Vereda, Murete y Mástil en Baja Tensión - Soles"]
[null,"Descripción",null,null,null,"Unidad","Costo"]
[null,"Rotura y resane de vereda en baja tensión",null,null,null,"m2",152]
[null,"Murete baja tensión, conexión monofásica",null,null,null,"Unidad",187]
[null,"Murete baja tensión, conexión trifásica",null,null,null,"Unidad",207]
[null,"Mástil metálico de 3 m",null,null,null,"Unidad",94]
[null,"Mástil metálico de 6 m",null,null,null,"Unidad",148]
[null,"Costos Adicionales al Sistema de Proteccion y Seccionamiento - Soles"]
[null,"Descripción",{"$nulls":6},"Unidad","Costo"]
[null,"Seccionador Tipo Expulsión, Exterior, Unipolar, Bajo Carga, 10kV, 300A x 3 (1)",{"$nulls":6},"Unidad",2204]
[null,"Seccionador Tipo Expulsión, Exterior, Unipolar, Bajo Carga, 22.9kV, 200A x 3 (1)",{"$nulls":6},"Unidad",3655]
[null,"Seccionador Bajo Carga, Interior, Tripolar, 10kV, 400A x 1 (2)",{"$nulls":6},"Unidad",6023]
[null,"Aislador Extensor, Polimerico, 25kv, Para Cut-Out x 3 (3)",{"$nulls":6},"Unidad",845]

{"sheet":"REP_MTTO","index":2,"n_rows":95,"n_cols":15,"rows_kept":95,"cut":false,"hidden":false,"merged":[[81,0,85,0],[81,1,85,1],[54,8,54,14],[62,5,62,6],[62,7,62,8],[62,9,62,10],[62,11,62,12],[32,0,32,4],[32,5,32,6],[32,7,32,8],[32,9,32,10],[32,11,32,12],[79,7,79,8],[79,9,79,10],[70,1,75,1],[70,2,73,2],[74,2,75,2],[79,0,79,4],[79,5,79,6],[1,0,1,14],[3,7,3,8],[3,9,3,10],[3,11,3,12],[3,13,3,14],[5,0,14,0],[5,1,14,1],[5,2,10,2],[5,3,10,3],[11,2,14,2],[11,3,14,3],[15,0,28,0],[15,1,22,1],[15,2,18,2],[15,3,18,3],[43,7,43,8],[25,1,28,1],[43,9,43,10],[43,11,43,12],[43,13,43,14],[19,2,22,2],[19,3,22,3]]}
[]
["CARGOS DE REPOSICION Y MANTENIMIENTO  DE LA CONEXIÓN ELECTRICA (NO INCLUYE IGV)"]
["Conexiones en Baja Tensión 220 V - Nuevos Soles",{"$nulls":6},"Vigente a partir del 04-04-2022"]
[{"$nulls":7},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT5A",1.7100000000000002,1.73]
[{"$nulls":4},"BT5B (2 hilos)",null,null,1.25,1.25,1.3,1.31,1.49,1.5,1.55,1.55]
[{"$nulls":4},"BT5B (2 hilos) - Rural (1)",null,null,1.44,null,1.51,null,1.75,null,1.82]
[{"$nulls":4},"BT5B (3 hilos)",null,null,1.25,1.25,1.3,1.31,1.49,1.5,1.55,1.55]
[{"$nulls":4},"BT5B (3 hilos) - Rural (1)",null,null,1.49,null,1.56,null,1.8,null,1.87]
[{"$nulls":4},"BT6",0.72,0.74]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT5A",1.7600000000000002,1.73]
[{"$nulls":4},"BT5B (2 hilos)",null,null,1.25,1.25,1.3,1.31,1.49,1.5,1.55,1.55]
[{"$nulls":4},"BT5B (3 hilos)",null,null,1.25,1.25,1.3,1.31,1.49,1.5,1.55,1.55]
[{"$nulls":4},"BT6",0.72,0.74]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5A",3.24,3.29]
[{"$nulls":4},"BT5B",null,null,1.72,1.7799999999999998,1.72,1.7799999999999998,1.86,1.9,1.86,1.9]
[{"$nulls":4},"BT6",0.79,0.79]
[{"$nulls":4},"BT2/BT3/BT4",3.7800000000000002,3.83]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5A",3.24,3.29]
[{"$nulls":4},"BT5B",null,null,1.72,1.7799999999999998,1.72,1.7799999999999998,1.86,1.9,1.86,1.9]
[{"$nulls":4},"BT6",0.79,0.79]
[{"$nulls":4},"BT2/BT3/BT4",3.83,3.88]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW","BT5B",5.2200000000000006,5.17]
[{"$nulls":4},"BT5A/BT2/BT3/BT4",5.2200000000000006,5.17]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW","BT2/BT3/BT4",5.29,5.42]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW","BT2/BT3/BT4",null,6.02]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW","BT2/BT3/BT4",null,6.68]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW","BT2/BT3/BT4",null,6.93]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.            (3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 220 V - Nuevos Soles"]
[{"$nulls":5},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT5B (2 hilos)",1.3,1.19,1.35,1.25,1.54,1.44,1.6,1.49]
[{"$nulls":4},"BT5B (3 hilos)",1.33,1.22,1.3800000000000001,1.28,1.57,1.47,1.6300000000000001,1.52]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT5B (2 hilos)",1.33,1.22,1.3800000000000001,1.28,1.57,1.47,1.6300000000000001,1.52]
[{"$nulls":4},"BT5B (3 hilos)",1.33,1.22,1.3800000000000001,1.28,1.57,1.47,1.6300000000000001,1.52]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5B",1.75,1.7,1.75,1.7,1.8900000000000001,1.82,1.8900000000000001,1.82]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5B",1.7999999999999998,1.75,1.7999999999999998,1.75,1.94,1.87,1.94,1.87]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión 380/220 V - Nuevos Soles"]
[{"$nulls":7},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5A",3.24,3.29]
[{"$nulls":4},"BT5B",null,null,1.72,1.81,1.72,1.81,1.86,1.9300000000000002,1.86,1.9300000000000002]
[{"$nulls":4},"BT6",0.79,0.84000000000000008]
[{"$nulls":4},"BT2/BT3/BT4",3.7800000000000002,3.83]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5A",3.24,3.29]
[{"$nulls":4},"BT5B",null,null,1.72,1.81,1.72,1.81,1.86,1.9300000000000002,1.86,1.9300000000000002]
[{"$nulls":4},"BT6",0.79,0.84000000000000008]
[{"$nulls":4},"BT2/BT3/BT4",3.7800000000000002,3.83]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW","BT5B",5.17,5.09]
[{"$nulls":4},"BT5A/BT2/BT3/BT4",5.17,5.09]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW","BT2/BT3/BT4",5.25,5.21]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW","BT2/BT3/BT4",null,5.62]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW","BT2/BT3/BT4",null,6.27]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW","BT2/BT3/BT4",null,6.52]
["(1) Aplicable a conexiones con acometida simple o doble."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 380/220 V - Nuevos Soles"]
[{"$nulls":5},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5B",1.75,1.7,1.75,1.7,1.8900000000000001,1.82,1.8900000000000001,1.82]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5B",1.7999999999999998,1.75,1.7999999999999998,1.75,1.94,1.87,1.94,1.87]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión 220 V - Prepago - Nuevos Soles"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea              (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT7 (2 hilos)",1.79,1.81]
[{"$nulls":4},"BT7 (2 hilos) - Rural (1)",1.79,0.72]
[{"$nulls":4},"BT7 (3 hilos)",2.35,2.27]
[{"$nulls":4},"BT7 (3 hilos) - Rural (1)",2.38,0.72]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT7 (2 hilos)",1.79,1.81]
[{"$nulls":4},"BT7 (3 hilos)",2.35,2.27]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.",null,null,null,"(3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Media Tensión - Nuevos Soles"]
[{"$nulls":5},"10 kV",null,"13.2/7.62 kV",null,"20 kV - 22.9/13.2 kV"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","PMI","Celda","PMI","Celda","PMI","Celda"]
["Trifásica","C5","C5.1","Pc ≤ 100 kW","MT2/MT3/MT4",18.490000000000002,26.52,19.23,28.69,20.490000000000002,31.35]
[null,null,"C5.2","100 kW < Pc ≤ 400 kW","MT2/MT3/MT4",19.72,25.880000000000003,19.27,27.87,20.490000000000002,31.35]
[null,null,"C5.3","400 kW < Pc ≤ 700 kW","MT2/MT3/MT4",19.23,25.65,19.38,27.57,20.76,32.32]
[null,null,"C5.4","700 kW < Pc ≤ 1000 kW","MT2/MT3/MT4",19.34,25.4,19.38,27.57,20.87,32.090000000000003]
[null,null,"C5.5","1000 kW < Pc ≤ 2500 kW","MT2/MT3/MT4",20.91,26.44,20.350000000000001,28.28,22.18,32.06]
{"$rows_empty":8}
["  "]

{"sheet":"COR_RECONEX","index":3,"n_rows":113,"n_cols":6,"rows_kept":113,"cut":false,"hidden":false,"merged":[[84,0,95,0],[100,0,107,0],[10,1,13,1],[15,4,15,5],[47,1,49,1],[24,0,24,3],[34,0,34,2],[34,3,35,3],[26,0,31,0],[28,1,29,1],[30,1,31,1],[45,0,45,3],[45,4,45,5],[47,0,52,0],[50,1,52,1],[36,0,43,0],[0,0,0,5],[1,0,1,5],[4,0,4,2],[4,3,5,3],[17,1,19,1],[6,0,13,0],[6,1,9,1],[17,0,22,0],[20,1,22,1],[36,1,39,1],[40,1,43,1],[66,0,79,0],[82,0,82,3],[82,4,82,5],[54,0,54,3],[54,4,54,5],[56,0,61,0],[58,1,59,1],[60,1,61,1],[64,0,64,3],[64,4,64,5],[112,0,112,1],[110,0,110,1],[111,0,111,1],[98,0,98,3],[98,4,98,5]]}
[]
["IMPORTES MAXIMOS DE CORTE Y RECONEXION (NO INCLUYE IGV)"]
["Conexiones monofásicas, hasta 10 kW, BT5A, BT5B y BT6"]
[null,null,"Vigente a partir del 04-04-2022"]
["Descripción",null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Fusible o interruptor (tapa sin ranura)",7.37]
[null,null,"Interruptor (tapa con ranura)",9.99]
[null,null,"Caja de medición (aislamiento acometida)",10.72]
[null,null,"Línea aérea (empalme)",25.64]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)",8.8800000000000008]
[null,null,"Interruptor (tapa con ranura)",11.48]
[null,null,"Caja de medición (aislamiento acometida)",12.31]
[null,null,"Línea aérea (empalme)",31.15]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Retiro","RT conexión aérea","Camioneta",51.5,55.22]
[null,null,"RT conexión subterránea","Camioneta",52.45,55.97]
[null,null,"RT conexión mixta","Camioneta",52.45,55.97]
[null,"Reinstalación","RIconexión aérea","Camioneta",91.03,98.06]
[null,null,"RI conexión subterránea","Camioneta",68.37,73.92]
[null,null,"RI conexión mixta","Camioneta",68.37,73.92]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Caja de medición (aislamiento acometida bloqueada)","Camioneta",23.66,27.63]
[null,"Reconexión","Caja de medición (aislamiento acometida bloqueada)","Camioneta",21.36,26.25]
[null,"Retiro","RT conexión subterránea (empalme y cable de acometida)","Camioneta",175.64,182.66]
[null,null,"RT conexión mixta (empalme y cable de acometida)","Camioneta",175.64,182.66]
[null,"Reinstalación","RI conexión subterránea (empalme y cable de acometida)","Camioneta",242.32,251.7]
[null,null,"RI conexión mixta (empalme y cable de acometida)","Camioneta",242.32,251.7]
[]
["Conexiones Trifásicas, hasta 20 kW, BT5A, BT5B y BT6"]
["Descripción",null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Fusible o interruptor (tapa sin ranura)",8.75]
[null,null,"Interruptor (tapa con ranura)",11.13]
[null,null,"Caja de medición (aislamiento acometida)",11.23]
[null,null,"Línea aérea (empalme)",25.38]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)",11.76]
[null,null,"Interruptor (tapa con ranura)",13.71]
[null,null,"Caja de medición (aislamiento acometida)",14.69]
[null,null,"Línea aérea (empalme)",32.03]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Retiro","RT conexión aérea","Camioneta",61.26,65.95]
[null,null,"RT conexión subterránea","Camioneta",56.92,60.43]
[null,null,"RT conexión mixta","Camioneta",56.92,60.43]
[null,"Reinstalación","RI conexión aérea","Camioneta",105.05,113.06]
[null,null,"RI conexión subterránea","Camioneta",76.7,82.94]
[null,null,"RI conexión mixta","Camioneta",76.7,82.94]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Caja de medición (aislamiento acometida bloqueada)","Camioneta",26.83,31.52]
[null,"Reconexión","Caja de medición (aislamiento acometida bloqueada)","Camioneta",28.9,32.56]
[null,"Retiro","RT conexión subterránea (empalme y cable de acometida)","Camioneta",192.74,199.77]
[null,null,"RT conexión mixta (empalme y cable de acometida)","Camioneta",192.74,199.77]
[null,"Reinstalación","RI conexión subterránea (empalme y cable de acometida)","Camioneta",282.99,282.99]
[null,null,"RI conexión mixta (empalme y cable de acometida)","Camioneta",273.64999999999998,281.87]
[]
["Conexiones Trifásicas, hasta 20 kW, resto de opciones (BT2,BT3 y BT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW resto de opciones (BT2,BT3 y BT4)","Corte","Fusible o interruptor (tapa sin ranura)","Camioneta",24.73,26.72]
[null,null,"Interruptor (tapa con ranura)","Camioneta",27.67,29.94]
[null,null,"Caja de medición (aislamiento acometida)","Camioneta",27.83,30.05]
[null,null,"Línea aérea (empalme)","Camioneta",39.619999999999997,42.44]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)","Camioneta",40.18,42.36]
[null,null,"Interruptor (tapa con ranura)","Camioneta",31.29,33.86]
[null,null,"Caja de medición (aislamiento acometida)","Camioneta",43.91,45.89]
[null,null,"Línea aérea (empalme)","Camioneta",59.47,62.41]
[null,"Retiro","RT conexión aérea","Camioneta",61.26,65.95]
[null,null,"RT conexión subterránea","Camioneta",56.92,60.43]
[null,null,"RT conexión mixta","Camioneta",56.92,60.43]
[null,"Reinstalación","RIconexión aérea","Camioneta",117.03,125.06]
[null,null,"RIión subterránea","Camioneta",88.69,94.97]
[null,null,"RI conexión mixta","Camioneta",88.69,94.97]
[]
["Conexiones trifásicas mayor a 20 kW, resto de opciones (BT2,BT3 y BT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica mayor a 20 kW resto de opciones (BT2,BT3 y BT4)","Corte","En fusible o interruptor (tapa sin ranura)","Camioneta",27.59,29.82]
[null,null,"En caja de medición (aislamiento acometida)","Camioneta",30.17,32.590000000000003]
[null,null,"En línea aérea (empalme)","Camioneta",44.82,47.84]
[null,"Reconexión","En fusible o interruptor (tapa sin ranura)","Camioneta",36.159999999999997,38.380000000000003]
[null,null,"En caja de medición (aislamiento acometida)","Camioneta",45.26,48.19]
[null,null,"En línea aérea (empalme)","Camioneta",72.459999999999994,76.459999999999994]
[null,"Retiro","En conexión aérea","Camioneta",89.33,96.31]
[null,null,"En conexión subterránea","Camioneta",83.65,89.88]
[null,null,"En conexión mixta","Camioneta",83.65,89.88]
[null,"Reinstalación","En conexión aérea","Camioneta",133.59,142.91]
[null,null,"En conexión subterránea","Camioneta",107.7,115.73]
[null,null,"En conexión mixta","Camioneta",107.7,115.73]
[]
["Conexiones trifásicas, hasta 2500 kW, resto de opciones (MT2,MT3 y MT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 2500 kW resto de opciones (MT2,MT3 y MT4)","Corte","En sistema de protección - PMI","Camioneta",56.22,60.9]
[null,null,"En sistema de protección - Celda","Camioneta",56.17,60.82]
[null,"Reconexión","En sistema de protección - PMI","Camioneta",56.17,60.82]
[null,null,"En sistema de protección - Celda","Camioneta",67.42,72.97]
[null,"Retiro","En sistema de protección - PMI","Camioneta",236.97,246.29]
[null,null,"En sistema de protección - Celda","Camioneta",96.24,104.25]
[null,"Reinstalación","En sistema de protección - PMI","Camioneta",419.43,430.66]
[null,null,"En sistema de protección - Celda","Camioneta",247.33,256.7]
[]
["Suministros Rurales con Celdas Fotovoltaicas (Sierra)"]
["Tipo",null,"Costo Total (S/.)"]
["Corte",null,8.0299999999999994]
["Reconexión",null,10.07]