{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["ENERGIA","CONEXION","REP_MTTO","COR_RECONEX"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ENERGIA","index":0,"n_rows":149,"n_cols":30,"rows_kept":149,"cut":false,"hidden":false,"merged":[[0,7,0,29],[1,0,1,1],[2,0,2,5],[146,7,146,12],[146,13,146,18]]}
["PLIEGO TARIFARIO DEL SERVICIO PUBLICO DE ELECTRICIDAD (NO INCLUYE IGV)"]
["2022-03-04",{"$nulls":14},"VIGENTE A PARTIR DEL DIA 04-03-2022"]
["SISTEMA ELECTRICO",{"$nulls":6},"Cusco","Valle Sagrado 1","Valle Sagrado 2","Valle Sagrado 3","Sicuani","Sicuani Rural","Combapata, Chumbivilcas","Yauri","La Convención, Macupicchu","La Convención Rural","Abancay","Abancay Rural, Chuquibambilla, Chacapuente","Andahuyalas","Puerto Maldonado","Puerto Maldonad Rural-Iñapari-Iberia","Mazuko","SER-Apurimac y Valle Sagrado","SER-Valle Vilcanota","SER-Quispicanchis","SER-Espinar","SER-Iberia","SER-Machupicchu","SER-Mazuko"]
["MEDIA TENSION",{"$nulls":5},"UNIDAD",{"$nulls":10},"TARIFA"]
["MT2","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",32.35,32.229999999999997,32.35,32.229999999999997,32.799999999999997,32.799999999999997,32.799999999999997,33.17,31.42,31.42,32.229999999999997,32.229999999999997,32.229999999999997,34.33,34.33,32.03,32.229999999999997,32.799999999999997,32.35,33.17,34.33,31.42,32.03]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",27,26.93,27,26.93,27.38,27.38,27.38,27.76,26.33,26.33,26.93,26.93,26.93,27.01,27.01,26.54,26.93,27.38,27,27.76,27.01,26.33,26.54]
[null,"Cargo por Potencia Activa de Generación en HP",{"$nulls":4},"S/./kW-mes",69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8,69.8]
[null,"Cargo por Potencia Activa por uso de redes de Distribución en HP",{"$nulls":4},"S/./kW-mes",21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62,21.62]
[null,"Cargo por Exceso de Potencia Activa por uso de redes de Distribución en HFP",{"$nulls":4},"S/./kW-mes",22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12,22.12]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01]
["MT3","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",32.35,32.229999999999997,32.35,32.229999999999997,32.799999999999997,32.799999999999997,32.799999999999997,33.17,31.42,31.42,32.229999999999997,32.229999999999997,32.229999999999997,34.33,34.33,32.03,32.229999999999997,32.799999999999997,32.35,33.17,34.33,31.42,32.03]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",27,26.93,27,26.93,27.38,27.38,27.38,27.76,26.33,26.33,26.93,26.93,26.93,27.01,27.01,26.54,26.93,27.38,27,27.76,27.01,26.33,26.54]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01]
["MT4","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14]
[null,"Cargo por Energía Activa",{"$nulls":4},"ctm.S/./kW.h",28.33,28.24,28.33,28.24,28.73,28.73,28.73,29.1,27.59,27.59,28.24,28.24,28.24,28.83,28.83,27.9,28.24,28.73,28.33,29.1,28.83,27.59,27.9]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73,63.73]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69,40.69]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14,23.14]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75,22.75]
[null,"Cargo por Energía Reactiva que Exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01]
["BAJA TENSION"]
["BT2","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25,13.25]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",35.1,34.97,35.1,34.97,35.590000000000003,35.590000000000003,35.590000000000003,35.99,34.090000000000003,34.090000000000003,34.97,34.97,34.97,37.26,37.26,34.75,34.97,35.590000000000003,35.1,35.99,37.26,34.090000000000003,34.75]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",29.3,29.21,29.3,29.21,29.71,29.71,29.71,30.13,28.56,28.56,29.21,29.21,29.21,29.32,29.32,28.8,29.21,29.71,29.3,30.13,29.32,28.56,28.8]
[null,"Cargo por Potencia Activa de Generación en HP",{"$nulls":4},"S/./kW-mes",72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994,72.209999999999994]
[null,"Cargo por Potencia Activa por uso de redes de Distribución en HP",{"$nulls":4},"S/./kW-mes",100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33,100.33]
[null,"Cargo por Exceso de Potencia Activa por uso de redes de Distribución en HFP",{"$nulls":4},"S/./kW-mes",73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006,73.790000000000006]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01]
["BT3","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",35.1,34.97,35.1,34.97,35.590000000000003,35.590000000000003,35.590000000000003,35.99,34.090000000000003,34.090000000000003,34.97,34.97,34.97,37.26,37.26,34.75,34.97,35.590000000000003,35.1,35.99,37.26,34.090000000000003,34.75]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",29.3,29.21,29.3,29.21,29.71,29.71,29.71,30.13,28.56,28.56,29.21,29.21,29.21,29.32,29.32,28.8,29.21,29.71,29.3,30.13,29.32,28.56,28.8]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72]
[null,"Cargo por Energía Reactiva que exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01]
["BT4","Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14]
[null,"Cargo por Energía Activa",{"$nulls":4},"ctm.S/./kW.h",30.74,30.64,30.74,30.64,31.18,31.18,31.18,31.57,29.94,29.94,30.64,30.64,30.64,31.28,31.28,30.27,30.64,31.18,30.74,31.57,31.28,29.94,30.27]
[null,"Cargo por Potencia Activa de Generación para Usuarios:",{"$nulls":4}," "]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88,50.88]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98,48.98]
[null,"Cargo por Potencia Activa por uso de resdes de Distribución para Usuarios:"]
[null,"           Presentes en Punta",{"$nulls":4},"S/./kW-mes",97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44,97.44]
[null,"           Presentes Fuera de Punta",{"$nulls":4},"S/./kW-mes",94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72,94.72]
[null,"Cargo por Energía Reactiva que Exceda el 30% del total de la Energía Activa",{"$nulls":4},"ctm.S/./kVar.h",5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01,5.01]
["BT5A","a) Usuarios con demanda maximia mensuakl de hasta 20KW en HP y HFP"]
[null,"Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",227.23,227.11,227.23,227.11,227.73,227.73,227.73,228.13,226.23,226.23,227.11,227.11,227.11,229.4,229.4,226.89,227.11,227.73,227.23,228.13,229.4,226.23,226.89]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",29.3,29.21,29.3,29.21,29.71,29.71,29.71,30.13,28.56,28.56,29.21,29.21,29.21,29.32,29.32,28.8,29.21,29.71,29.3,30.13,29.32,28.56,28.8]
[null,"Cargo por Exceso de Potencia en HFP",{"$nulls":4},"S/.kW-mes",91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16]
[null,"b) Usuarios con demanda maximia mensuakl de hasta 20KW en HP y 50KW en HFP"]
[null,"Cargo Fijo Mensual",{"$nulls":4},"S/./mes",12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14]
[null,"Cargo por Energía Activa en Horas de Punta",{"$nulls":4},"ctm.S/./kW.h",269.69,269.55,269.69,269.55,270.18,270.18,270.18,270.58,268.67,268.67,269.55,269.55,269.55,271.83999999999997,271.83999999999997,269.33,269.55,270.18,269.69,270.58,271.83999999999997,268.67,269.33]
[null,"Cargo por Energía Activa en Horas Fuera de Punta",{"$nulls":4},"ctm.S/./kW.h",29.3,29.21,29.3,29.21,29.71,29.71,29.71,30.13,28.56,28.56,29.21,29.21,29.21,29.32,29.32,28.8,29.21,29.71,29.3,30.13,29.32,28.56,28.8]
[null,"Cargo por Exceso de Potencia en HFP",{"$nulls":4},"S/.kW-mes",91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16,91.16]
["BT5B","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09]
[null,"           Cargo por energía activa",null,null,"   ",null,"ctm.S/./kW.h",57.61,38.409999999999997,38.409999999999997,38.409999999999997,57.61,38.409999999999997,38.409999999999997,38.409999999999997,57.61,38.409999999999997,57.61,38.409999999999997,38.409999999999997,57.61,38.409999999999997,57.61,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",17.28,11.52,11.52,11.52,17.28,11.52,11.52,11.52,17.28,11.52,17.28,11.52,11.52,17.28,11.52,17.28,11.52,11.52,11.52,11.52,11.52,11.52,11.52]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993]
[null,"c) No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",84.11,84.01,84.11,84.01,84.54,84.54,84.54,84.95,83.31,83.31,84.01,84.01,84.01,84.65,84.65,83.65,84.01,84.54,84.11,84.95,84.65,83.31,83.65]
["BT5C-AP","           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996,4.8499999999999996]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",82.73,82.63,82.73,82.63,83.14,83.14,83.14,83.53,81.96,81.96,82.63,82.63,82.63,83.25,83.25,82.28,82.63,83.14,82.73,83.53,83.25,81.96,82.28]
["BT5D","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",43.05,28.66,28.7,28.66,43.34,28.89,28.89,29.08,42.51,28.34,42.98,28.66,28.66,43.42,28.95,42.74,28.66,28.89,28.7,29.08,28.95,28.34,28.49]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09,4.09]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",12.92,8.6,8.61,8.6,13,8.67,8.67,8.7200000000000006,12.75,8.5,12.89,8.6,8.6,13.03,8.68,12.82,8.6,8.67,8.61,8.7200000000000006,8.68,8.5,8.5500000000000007]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",57.4,57.31,57.4,57.31,57.78,57.78,57.78,58.15,56.68,56.68,57.31,57.31,57.31,57.89,57.89,56.98,57.31,57.78,57.4,58.15,57.89,56.68,56.98]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",60.21,60.12,60.21,60.12,60.61,60.61,60.61,61,59.46,59.46,60.12,60.12,60.12,60.73,60.73,59.77,60.12,60.61,60.21,61,60.73,59.46,59.77]
[null,"c)  No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",60.21,60.12,60.21,60.12,60.61,60.61,60.61,61,59.46,59.46,60.12,60.12,60.12,60.73,60.73,59.77,60.12,60.61,60.21,61,60.73,59.46,59.77]
["BT6","Cargo Fijo Mensual - Lectura Mensual",{"$nulls":4},"S/./mes",4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29,4.29]
[null,"Cargo por Potencia",{"$nulls":4},"cent. S/./W",31.8,31.75,31.8,31.75,31.95,31.95,31.95,32.11,31.49,31.49,31.75,31.75,31.75,32,32,31.62,31.75,31.95,31.8,32.11,32,31.49,31.62]
["BT7","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",57.61,38.409999999999997,38.409999999999997,38.409999999999997,57.61,38.409999999999997,38.409999999999997,38.409999999999997,57.61,38.409999999999997,57.61,38.409999999999997,38.409999999999997,57.61,38.409999999999997,57.61,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997]
[null,"31-100 kWh"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28,3.28]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",17.28,11.52,11.52,11.52,17.28,11.52,11.52,11.52,17.28,11.52,17.28,11.52,11.52,17.28,11.52,17.28,11.52,11.52,11.52,11.52,11.52,11.52,11.52]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993]
[null,"c)  No Residencial"]
[null,"           Cargo Comercial del Servicio Prepago",{"$nulls":4},"S/./mes",3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44,3.44]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",82.87,82.78,82.87,82.78,83.3,83.3,83.3,83.7,82.08,82.08,82.78,82.78,82.78,83.42,83.42,82.41,82.78,83.3,82.87,83.7,83.42,82.08,82.41]
["BT5E","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",57.61,38.409999999999997,38.409999999999997,38.409999999999997,57.61,38.409999999999997,38.409999999999997,38.409999999999997,57.61,38.409999999999997,57.61,38.409999999999997,38.409999999999997,57.61,38.409999999999997,57.61,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997]
[null,"31-100 kWh"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57,2.57]
[null,"           Cargo por energía activa-Primeros 30 kWh",{"$nulls":4},"S/./mes",17.28,11.52,11.52,11.52,17.28,11.52,11.52,11.52,17.28,11.52,17.28,11.52,11.52,17.28,11.52,17.28,11.52,11.52,11.52,11.52,11.52,11.52,11.52]
[null,"           Cargo por energía activa-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993]
[null,"c)  No Residencial"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7,2.7]
[null,"           Cargo por energía activa",{"$nulls":4},"ctm.S/./kW.h",84.09,83.99,84.09,83.99,84.52,84.52,84.52,84.93,83.28,83.28,83.99,83.99,83.99,84.63,84.63,83.62,83.99,84.52,84.09,84.93,84.63,83.28,83.62]
["BT5F","a) Residencial con consumo menor o iguales a 100 kW.h por mes"]
[null,"0-30 kWh"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",57.61,38.409999999999997,38.409999999999997,38.409999999999997,57.61,38.409999999999997,38.409999999999997,38.409999999999997,57.61,38.409999999999997,57.61,38.409999999999997,38.409999999999997,57.61,38.409999999999997,57.61,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",43.14,28.72,28.76,28.72,43.43,28.96,28.96,29.15,42.62,28.41,43.08,28.72,28.72,43.15,28.77,42.77,28.72,28.96,28.76,29.15,28.77,28.41,28.52]
[null,"31-100 kWh"]
[null,"         Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2,4.2]
[null,"         Cargo por energía activa Hora Punta-Primeros 30 kWh",{"$nulls":4},"ctm.S/./kW.h",57.61,38.409999999999997,38.409999999999997,38.409999999999997,57.61,38.409999999999997,38.409999999999997,38.409999999999997,57.61,38.409999999999997,57.61,38.409999999999997,38.409999999999997,57.61,38.409999999999997,57.61,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997,38.409999999999997]
[null,"         Cargo por energía activa Fuera de Punta-Primeros 30 kWh",{"$nulls":4},"ctm.S/./kW.h",43.14,28.72,28.76,28.72,43.43,28.96,28.96,29.15,42.62,28.41,43.08,28.72,28.72,43.15,28.77,42.77,28.72,28.96,28.76,29.15,28.77,28.41,28.52]
[null,"         Cargo por energía activa Hora Punta-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81,76.81]
[null,"         Cargo por energía activa Fuera de Punta-Exceso de 30 kWh",{"$nulls":4},"ctm.S/./kW.h",57.52,57.44,57.52,57.44,57.91,57.91,57.91,58.3,56.82,56.82,57.44,57.44,57.44,57.53,57.53,57.03,57.44,57.91,57.52,58.3,57.53,56.82,57.03]
[null,"b) Residencial con consumo mayor 100 kW.h por mes"]
[null,"           Cargo Fijo Mensual",{"$nulls":4},"S/./mes",4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41,4.41]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993,80.569999999999993]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",60.34,60.25,60.34,60.25,60.75,60.75,60.75,61.16,59.6,59.6,60.25,60.25,60.25,60.35,60.35,59.82,60.25,60.75,60.34,61.16,60.35,59.6,59.82]
[null,"c) No Residencial"]
[null,"           Cargo Fijo Mensual ",{"$nulls":4},"S/./mes",12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14,12.14]
[null,"           Cargo por energía activa en horas de punta",{"$nulls":4},"ctm.S/./kW.h",130.1,129.97,130.1,129.97,130.6,130.6,130.6,131,129.09,129.09,129.97,129.97,129.97,132.26,132.26,129.75,129.97,130.6,130.1,131,132.26,129.09,129.75]
[null,"           Cargo por energía activa en horas fuera de punta",{"$nulls":4},"ctm.S/./kW.h",60.34,60.25,60.34,60.25,60.75,60.75,60.75,61.16,59.6,59.6,60.25,60.25,60.25,60.35,60.35,59.82,60.25,60.75,60.34,61.16,60.35,59.6,59.82]
["BT8","SUMINISTROS RURALES CON CELDAS FOTOVOLTAICAS (Sierra)",{"$nulls":5},"Inversion 100% Estado",{"$nulls":5},"Inversion 100% Empresa",{"$nulls":5},"  "]
[null,"Tipo de Módulo",{"$nulls":5},"BT8-070","BT8-100","BT8-160","BT8-240","BT8-320","BT8-050-Pre","BT8-070","BT8-100","BT8-160","BT8-240","BT8-320","BT8-050-Pre"]
[null,"Cargo Fijo Equivalente por Energia Promedio",{"$nulls":4},"ctm.S/./kW.h",93.99,81.19,59.61,52.01,81.099999999999994,121.71,153.49,131.41999999999999,97.41,86.69,135.91999999999999,161.5]

{"sheet":"CONEXION","index":1,"n_rows":131,"n_cols":11,"rows_kept":131,"cut":false,"hidden":false,"merged":[[0,0,0,10],[58,3,58,4],[58,5,58,6],[44,5,44,6],[45,5,45,6],[46,5,46,6],[50,5,50,6],[51,3,51,4],[51,5,51,6],[41,3,41,4],[41,5,41,6],[50,3,50,4],[52,5,52,6],[53,3,53,4],[43,5,43,6],[49,5,49,6],[52,3,52,4],[53,5,53,6],[47,5,47,6],[48,5,48,6],[32,3,32,4],[32,5,32,6],[37,3,37,4],[34,5,34,6],[36,5,36,6],[37,5,37,6],[35,5,35,6],[33,5,33,6],[40,3,40,4],[40,5,40,6],[128,1,128,7],[129,1,129,7],[130,1,130,7],[121,1,121,4],[122,1,122,4],[123,1,123,4],[124,1,124,4],[120,1,120,4],[127,1,127,7],[117,5,117,7],[114,5,114,7],[111,5,111,7],[112,5,112,7],[115,0,115,1],[115,5,115,7],[116,0,116,1],[116,5,116,7],[114,0,114,1],[114,2,114,4],[111,0,111,1],[113,0,113,1],[110,3,110,4],[110,5,110,7],[107,3,107,4],[107,5,107,7],[108,3,108,4],[108,5,108,7],[113,5,113,7],[109,3,109,4],[109,5,109,7],[113,2,113,4],[75,5,75,6],[64,5,64,6],[65,5,65,6],[59,5,59,6],[104,0,104,1],[106,3,106,4],[106,5,106,7],[103,3,103,4],[103,5,103,7],[104,3,104,4],[104,5,104,7],[96,5,96,7],[93,5,93,7],[94,3,94,4],[94,5,94,7],[93,3,93,4],[100,5,100,7],[101,5,101,7],[102,3,102,4],[102,5,102,7],[97,5,97,7],[98,5,98,7],[99,5,99,7],[26,5,26,6],[23,5,23,6],[41,0,53,0],[41,1,48,1],[41,2,44,2],[89,5,89,7],[91,5,91,7],[88,0,88,1],[88,3,88,4],[88,5,88,7],[66,5,66,6],[67,5,67,6],[68,5,68,6],[76,3,76,4],[76,5,76,6],[90,5,90,7],[67,3,67,4],[74,3,74,4],[74,5,74,6],[78,0,78,4],[78,5,78,6],[78,7,78,8],[42,5,42,6],[62,3,62,4],[4,5,4,6],[23,3,23,4],[5,5,5,6],[11,5,11,6],[6,5,6,6],[12,5,12,6],[13,5,13,6],[16,5,16,6],[25,3,25,4],[25,5,25,6],[24,3,24,4],[24,5,24,6],[20,5,20,6],[21,5,21,6],[22,5,22,6],[7,5,7,6],[8,5,8,6],[9,5,9,6],[10,5,10,6],[19,5,19,6],[14,5,14,6],[15,5,15,6],[17,5,17,6],[18,5,18,6],[14,0,26,0],[14,1,21,1],[14,2,17,2],[14,3,14,4],[18,2,21,2],[18,3,18,4],[22,3,22,4],[23,1,26,1],[4,3,4,4],[26,3,26,4],[119,1,119,4],[126,1,126,7],[45,2,48,2],[45,3,45,4],[49,3,49,4],[50,1,53,1],[57,3,57,4],[57,5,57,6],[58,0,59,0],[58,1,59,1],[94,0,94,1],[97,3,97,4],[100,3,100,4],[62,5,62,6],[59,3,59,4],[105,3,105,4],[105,5,105,7],[101,3,101,4],[92,5,92,7],[95,5,95,7],[102,0,102,1],[63,3,63,4],[63,5,63,6],[75,3,75,4],[1,0,1,8],[3,3,3,4],[3,5,3,6],[78,9,78,10],[87,0,87,1],[87,3,87,4],[87,5,87,7],[90,3,90,4],[92,3,92,4],[31,3,31,4],[31,5,31,6],[32,0,35,0],[32,1,35,1],[32,2,33,2],[34,2,35,2],[34,3,34,4],[36,0,37,0],[36,1,37,1],[36,3,36,4],[4,0,13,0],[4,1,13,1],[4,2,9,2],[10,2,13,2],[10,3,10,4]]}
[]
["PRESUPUESTOS DE LA CONEXIÓN ELECTRICA (NO INCLUYE IGV)"]
["Conexiones en Baja Tensión 220 V - Soles",{"$nulls":5},"Vigente a partir del 04-02-2022"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Aérea (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT5A",null,1097,1230]
[{"$nulls":5},"BT5B (2 hilos)",null,319,449]
[{"$nulls":5},"BT5B (2 hilos) - Rural (1)",null,366]
[{"$nulls":5},"BT5B (3 hilos)",null,326,459]
[{"$nulls":5},"BT5B (3 hilos) - Rural (1)",null,373]
[{"$nulls":5},"BT6",null,236,382]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT5A",null,1126,1237]
[{"$nulls":5},"BT5B (2 hilos)",null,349,459]
[{"$nulls":5},"BT5B (3 hilos)",null,355,466]
[{"$nulls":5},"BT6",null,265,387]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5A",null,2087,2217]
[{"$nulls":5},"BT5B",null,603,734]
[{"$nulls":5},"BT6",null,412,499]
[{"$nulls":5},"BT2/BT3/BT4",null,2618,2706]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5A",null,2118,2227]
[{"$nulls":5},"BT5B",null,634,743]
[{"$nulls":5},"BT6",null,442,510]
[{"$nulls":5},"BT2/BT3/BT4",null,2785,2853]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW",null,"BT5A/BT5B/BT2/BT3/BT4",null,3561,3866]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW",null,"BT2/BT3/BT4",null,3809,4630]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW",null,"BT2/BT3/BT4",null,null,6490]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW",null,"BT2/BT3/BT4",null,null,8554]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW",null,"BT2/BT3/BT4",null,null,9376]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.            (3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
[]
["Conexiones en Baja Tensión Múltiples 220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Conexión","Caja toma (1)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT5B (2 hilos)",null,186,82]
[{"$nulls":5},"BT5B (3 hilos)",null,191,82]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT5B (2 hilos)",null,202,145]
[{"$nulls":5},"BT5B (3 hilos)",null,209,145]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5B",null,387,146]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5B",null,413,299]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["Conexiones en Baja Tensión 380/220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                       Tarifaria",null,"Aérea            (1)","Subterránea (1)(2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5A",null,2135,2311]
[{"$nulls":5},"BT5B",null,609,786]
[{"$nulls":5},"BT6",null,419,548]
[{"$nulls":5},"BT2/BT3/BT4",null,2617,2746]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5A",null,2139,2316]
[{"$nulls":5},"BT5B",null,613,790]
[{"$nulls":5},"BT6",null,422,552]
[{"$nulls":5},"BT2/BT3/BT4",null,2620,2751]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW",null,"BT5A/BT5B/BT2/BT3/BT4",null,3363,3696]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW",null,"BT2/BT3/BT4",null,3603,4062]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW",null,"BT2/BT3/BT4",null,null,5238]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW",null,"BT2/BT3/BT4",null,null,7330]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW",null,"BT2/BT3/BT4",null,null,8033]
["(1) Aplicable a conexiones con acometida simple o doble."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 380/220 V - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Conexión","Caja Toma (1)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW",null,"BT5B",null,385,121]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW",null,"BT5B",null,389,270]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["Conexiones en Baja Tensión 220 V - Prepago - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Aérea            (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT7 (2 hilos)",null,692,825]
[{"$nulls":5},"BT7 (2 hilos) - Rural (1)",null,740]
[{"$nulls":5},"BT7 (3 hilos)",null,963,830]
[{"$nulls":5},"BT7 (3 hilos) - Rural (1)",null,1010]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT7 (2 hilos)",null,721,831]
[{"$nulls":5},"BT7 (3 hilos)",null,993,846]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble."]
["(3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
[]
["Costo por Metro de Cable de Conexiones en Baja Tensión 220 V - Prepago - Soles"]
["Fases","Tipo","Subtipo","Potencia                                      Conectada (Pc)",null,"Opción                                 Tarifaria",null,"Costo"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW",null,"BT7",null,5]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW",null,"BT7",null,6]
[]
["Conexiones Básicas en Media Tensión - Soles",{"$nulls":4},"10 kV",null,"13.2/7.62 kV",null,"20 kV - 22.9/13.2 kV"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","PMI","Celda","PMI","Celda","PMI","Celda"]
["Trifásica","C5","C5.1","Pc ≤ 100 kW","MT2/MT3/MT4",11372,19436,13951,25390,15688,25427]
[null,null,"C5.2","100 kW < Pc ≤ 400 kW","MT2/MT3/MT4",15208,17485,14034,22797,15688,25427]
[null,null,"C5.3","400 kW < Pc ≤ 700 kW","MT2/MT3/MT4",13658,16717,14425,21775,16456,28457]
[null,null,"C5.4","700 kW < Pc ≤ 1000 kW","MT2/MT3/MT4",14105,15879,14425,21775,16819,27762]
[null,null,"C5.5","1000 kW < Pc ≤ 2500 kW","MT2/MT3/MT4",17224,16606,15729,21436,18449,25830]
[]
["Otros Elementos Electromecánicos en Media Tensión - Soles"]
["Elemento",null,"Tipo de red","Potencia Conectada (Pc)",null,"Descripción",null,null,"10 kV","13.2/7.62 kV","20 kV - 22.9/13.2 kV"]
["Empalme de acometida",null,"Aérea","Pc ≤ 1000 kW",null,"A red aérea con cable autoportante",null,null,1276,1106,1058]
[{"$nulls":5},"A red aérea con conductor desnudo",null,null,196,196,196]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"A red aérea con cable autoportante",null,null,1276,1106,1058]
[{"$nulls":5},"A red aérea con conductor desnudo",null,null,196,196,196]
[null,null,"Subterránea","Pc ≤ 1000 kW",null,"A red subterránea",null,null,7230,7230,7230]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"A red subterránea",null,null,7230,7230,7230]
["Cable de acometida",null,"Aérea","Pc ≤ 1000 kW",null,"Con cable autoportante y salida a red subterránea",null,null,7565,7225,7336]
[{"$nulls":5},"Con conductor desnudo y salida a red aérea",null,null,6152,6165,6495]
[{"$nulls":5},"Con conductor desnudo y salida a red subterránea",null,null,6297,6138,6177]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con cable autoportante y salida a red subterránea",null,null,7981,7225,7336]
[{"$nulls":5},"Con conductor desnudo y salida a red aérea",null,null,7095,6219,6495]
[{"$nulls":5},"Con conductor desnudo y salida a red subterránea",null,null,6945,6192,6177]
[null,null,"Subterránea-Aérea","Pc ≤ 1000 kW",null,"Con conductor desnudo y salida a red subterránea",null,null,7303,6963,7744]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con conductor desnudo y salida a red subterránea",null,null,7892,6963,7744]
["Caja de protección",null,"Subterránea","Pc ≤ 1000 kW",null,"Para celda interior",null,null,7082,6820,7055]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Para celda interior",null,null,7082,6820,7055]
["Sistema de protección y seccionamiento",null,"Aérea","Pc ≤ 100 kW",null,"Con seccionador cut-out",null,null,1701,1593,1791]
[null,null,null,"100 kW < Pc ≤ 400 kW",null,"Con seccionador cut-out",null,null,1706,1588,1792]
[null,null,null,"400 kW < Pc ≤ 700 kW",null,"Con seccionador cut-out",null,null,1727,1606,1792]
[null,null,null,"700 kW < Pc ≤ 1000 kW",null,"Con seccionador cut-out",null,null,1765,1623,1796]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con seccionador cut-out",null,null,7370,6566,7052]
[null,null,"Subterránea","Pc ≤ 1000 kW",null,"Con seccionador de potencia para celda interior",null,null,19378,20293,26019]
[null,null,null,"1000 kW < Pc ≤ 2500 kW",null,"Con seccionador de potencia para celda interior",null,null,31089,32108,25883]
["Protección sobretensión",null,"Aérea",null,null,"Para instalación exterior",null,null,1027,1093,1381]
[null,null,"Subterránea",null,null,"Para instalación interior",null,null,1633,1977,2231]
["Zanja (metro lineal)",null,"Aérea/Subterránea",null,null,"Para PMI o celda interior",null,null,61,61,61]
["Rotura y reparación de vereda (m2)",null,"Aérea/Subterránea",null,null,"Para PMI o celda interior",null,null,148,148,148]
["Murete",null,"Aérea",null,null,"Para PMI",null,null,317,317,317]
["Protección de estructuras",null,"Aérea",null,null,"Bloque de concreto",null,null,540,540,540]
[{"$nulls":5},"Riel de acero",null,null,176,176,176]
[null,"Costo por Vereda, Murete y Mástil en Baja Tensión - Soles"]
[null,"Descripción",null,null,null,"Unidad","Costo"]
[null,"Rotura y resane de vereda en baja tensión",null,null,null,"m2",148]
[null,"Murete baja tensión, conexión monofásica",null,null,null,"Unidad",183]
[null,"Murete baja tensión, conexión trifásica",null,null,null,"Unidad",202]
[null,"Mástil metálico de 3 m",null,null,null,"Unidad",92]
[null,"Mástil metálico de 6 m",null,null,null,"Unidad",145]
[null,"Costos Adicionales al Sistema de Proteccion y Seccionamiento - Soles"]
[null,"Descripción",{"$nulls":6},"Unidad","Costo"]
[null,"Seccionador Tipo Expulsión, Exterior, Unipolar, Bajo Carga, 10kV, 300A x 3 (1)",{"$nulls":6},"Unidad",2213]
[null,"Seccionador Tipo Expulsión, Exterior, Unipolar, Bajo Carga, 22.9kV, 200A x 3 (1)",{"$nulls":6},"Unidad",3670]
[null,"Seccionador Bajo Carga, Interior, Tripolar, 10kV, 400A x 1 (2)",{"$nulls":6},"Unidad",6047]
[null,"Aislador Extensor, Polimerico, 25kv, Para Cut-Out x 3 (3)",{"$nulls":6},"Unidad",848]

{"sheet":"REP_MTTO","index":2,"n_rows":95,"n_cols":15,"rows_kept":95,"cut":false,"hidden":false,"merged":[[15,0,28,0],[15,1,22,1],[15,2,18,2],[15,3,18,3],[43,7,43,8],[25,1,28,1],[43,9,43,10],[43,11,43,12],[43,13,43,14],[19,2,22,2],[19,3,22,3],[1,0,1,14],[3,7,3,8],[3,9,3,10],[3,11,3,12],[3,13,3,14],[5,0,14,0],[5,1,14,1],[5,2,10,2],[5,3,10,3],[11,2,14,2],[11,3,14,3],[81,0,85,0],[81,1,85,1],[54,8,54,14],[62,5,62,6],[62,7,62,8],[62,9,62,10],[62,11,62,12],[32,0,32,4],[32,5,32,6],[32,7,32,8],[32,9,32,10],[32,11,32,12],[79,7,79,8],[79,9,79,10],[70,1,75,1],[70,2,73,2],[74,2,75,2],[79,0,79,4],[79,5,79,6]]}
[]
["CARGOS DE REPOSICION Y MANTENIMIENTO  DE LA CONEXIÓN ELECTRICA (NO INCLUYE IGV)"]
["Conexiones en Baja Tensión 220 V - Nuevos Soles",{"$nulls":6},"Vigente a partir del 04-02-2022"]
[{"$nulls":7},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)","Aérea                       (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT5A",1.69,1.72]
[{"$nulls":4},"BT5B (2 hilos)",null,null,1.23,1.25,1.29,1.2999999999999998,1.47,1.4899999999999998,1.53,1.54]
[{"$nulls":4},"BT5B (2 hilos) - Rural (1)",null,null,1.42,null,1.49,null,1.72,null,1.79]
[{"$nulls":4},"BT5B (3 hilos)",null,null,1.23,1.25,1.29,1.2999999999999998,1.47,1.4899999999999998,1.53,1.54]
[{"$nulls":4},"BT5B (3 hilos) - Rural (1)",null,null,1.47,null,1.54,null,1.77,null,1.84]
[{"$nulls":4},"BT6",0.71,0.73]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT5A",1.7400000000000002,1.72]
[{"$nulls":4},"BT5B (2 hilos)",null,null,1.23,1.25,1.29,1.2999999999999998,1.47,1.4899999999999998,1.53,1.54]
[{"$nulls":4},"BT5B (3 hilos)",null,null,1.23,1.25,1.29,1.2999999999999998,1.47,1.4899999999999998,1.53,1.54]
[{"$nulls":4},"BT6",0.71,0.73]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5A",3.21,3.2600000000000002]
[{"$nulls":4},"BT5B",null,null,1.7,1.77,1.7,1.77,1.84,1.8900000000000001,1.84,1.8900000000000001]
[{"$nulls":4},"BT6",0.78,0.78]
[{"$nulls":4},"BT2/BT3/BT4",3.7399999999999998,3.8]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5A",3.21,3.2600000000000002]
[{"$nulls":4},"BT5B",null,null,1.7,1.77,1.7,1.77,1.84,1.8900000000000001,1.84,1.8900000000000001]
[{"$nulls":4},"BT6",0.78,0.78]
[{"$nulls":4},"BT2/BT3/BT4",3.79,3.8499999999999996]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW","BT5B",5.18,5.1400000000000006]
[{"$nulls":4},"BT5A/BT2/BT3/BT4",5.18,5.1400000000000006]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW","BT2/BT3/BT4",5.25,5.3900000000000006]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW","BT2/BT3/BT4",null,6]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW","BT2/BT3/BT4",null,6.68]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW","BT2/BT3/BT4",null,6.92]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.            (3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 220 V - Nuevos Soles"]
[{"$nulls":5},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT5B (2 hilos)",1.28,1.1800000000000002,1.34,1.23,1.52,1.42,1.58,1.47]
[{"$nulls":4},"BT5B (3 hilos)",1.32,1.22,1.3800000000000001,1.27,1.56,1.46,1.62,1.51]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT5B (2 hilos)",1.32,1.22,1.3800000000000001,1.27,1.56,1.46,1.62,1.51]
[{"$nulls":4},"BT5B (3 hilos)",1.32,1.22,1.3800000000000001,1.27,1.56,1.46,1.62,1.51]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5B",1.74,1.69,1.74,1.69,1.8800000000000001,1.81,1.8800000000000001,1.81]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5B",1.79,1.7399999999999998,1.79,1.7399999999999998,1.9300000000000002,1.8599999999999999,1.9300000000000002,1.8599999999999999]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión 380/220 V - Nuevos Soles"]
[{"$nulls":7},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)","Aérea                       (1)","Subterránea (2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5A",3.21,3.2600000000000002]
[{"$nulls":4},"BT5B",null,null,1.7,1.81,1.7,1.81,1.84,1.9300000000000002,1.84,1.9300000000000002]
[{"$nulls":4},"BT6",0.78,0.83000000000000007]
[{"$nulls":4},"BT2/BT3/BT4",3.7399999999999998,3.8]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5A",3.21,3.2600000000000002]
[{"$nulls":4},"BT5B",null,null,1.7,1.81,1.7,1.81,1.84,1.9300000000000002,1.84,1.9300000000000002]
[{"$nulls":4},"BT6",0.78,0.83000000000000007]
[{"$nulls":4},"BT2/BT3/BT4",3.7399999999999998,3.8]
[null,"C3","C3.1","20 kW < Pc ≤ 50 kW","BT5B",5.13,5.0600000000000005]
[{"$nulls":4},"BT5A/BT2/BT3/BT4",5.13,5.0600000000000005]
[null,"C4","C4.1","50 kW < Pc ≤ 75 kW","BT2/BT3/BT4",5.21,5.18]
[null,null,"C4.2","75 kW < Pc ≤ 150 kW","BT2/BT3/BT4",null,5.6]
[null,null,"C4.3","150 kW < Pc ≤ 225 kW","BT2/BT3/BT4",null,6.26]
[null,null,"C4.4","225 kW < Pc ≤ 300 kW","BT2/BT3/BT4",null,6.5]
["(1) Aplicable a conexiones con acometida simple o doble."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión Múltiples 380/220 V - Nuevos Soles"]
[{"$nulls":5},"Electrónico - Caja Plástico",null,"Electrónico - Caja Metal",null,"Electromecánico - Caja Plástico",null,"Electromecánico - Caja Metal"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)","Aérea                       (1)","Subterránea (1)(2)"]
["Trifásica","C2","C2.1","Pc ≤ 10 kW","BT5B",1.74,1.69,1.74,1.69,1.8800000000000001,1.81,1.8800000000000001,1.81]
[null,null,"C2.2","10 kW < Pc ≤ 20 kW","BT5B",1.79,1.7399999999999998,1.79,1.7399999999999998,1.9300000000000002,1.8599999999999999,1.9300000000000002,1.8599999999999999]
["(1) Aplicable en conexiones múltiples con 3 o más usuarios."]
["(2) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Baja Tensión 220 V - Prepago - Nuevos Soles"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","Aérea              (2)","Subterránea (2)(3)"]
["Monofásica","C1","C1.1","Pc ≤ 3 kW","BT7 (2 hilos)",1.7999999999999998,1.82]
[{"$nulls":4},"BT7 (2 hilos) - Rural (1)",1.7999999999999998,0.71]
[{"$nulls":4},"BT7 (3 hilos)",2.36,2.29]
[{"$nulls":4},"BT7 (3 hilos) - Rural (1)",2.4,0.71]
[null,null,"C1.2","3 kW < Pc ≤ 10 kW","BT7 (2 hilos)",1.7999999999999998,1.82]
[{"$nulls":4},"BT7 (3 hilos)",2.36,2.29]
["(1) Aplicable a los Sectores Típicos 3 , 4 y Sistemas Electricos Rurales (SER)"]
["(2) Aplicable a conexiones con acometida simple o doble.",null,null,null,"(3) Aplicable a conexiones subterráneas o mixtas (aérea/subterránea)."]
["Conexiones en Media Tensión - Nuevos Soles"]
[{"$nulls":5},"10 kV",null,"13.2/7.62 kV",null,"20 kV - 22.9/13.2 kV"]
["Fases","Tipo","Subtipo","Potencia Conectada (Pc)","Opción Tarifaria","PMI","Celda","PMI","Celda","PMI","Celda"]
["Trifásica","C5","C5.1","Pc ≤ 100 kW","MT2/MT3/MT4",18.48,26.74,19.240000000000002,28.97,20.509999999999998,31.67]
[null,null,"C5.2","100 kW < Pc ≤ 400 kW","MT2/MT3/MT4",19.740000000000002,26.09,19.29,28.13,20.509999999999998,31.67]
[null,null,"C5.3","400 kW < Pc ≤ 700 kW","MT2/MT3/MT4",19.240000000000002,25.85,19.399999999999999,27.82,20.79,32.67]
[null,null,"C5.4","700 kW < Pc ≤ 1000 kW","MT2/MT3/MT4",19.36,25.58,19.399999999999999,27.82,20.9,32.44]
[null,null,"C5.5","1000 kW < Pc ≤ 2500 kW","MT2/MT3/MT4",20.95,26.619999999999997,20.36,28.52,22.22,32.380000000000003]
{"$rows_empty":8}
["  "]

{"sheet":"COR_RECONEX","index":3,"n_rows":113,"n_cols":6,"rows_kept":113,"cut":false,"hidden":false,"merged":[[98,4,98,5],[34,0,34,2],[34,3,35,3],[17,1,19,1],[47,1,49,1],[45,0,45,3],[26,0,31,0],[28,1,29,1],[30,1,31,1],[47,0,52,0],[50,1,52,1],[54,0,54,3],[54,4,54,5],[56,0,61,0],[58,1,59,1],[60,1,61,1],[6,0,13,0],[6,1,9,1],[10,1,13,1],[0,0,0,5],[1,0,1,5],[4,0,4,2],[4,3,5,3],[15,4,15,5],[17,0,22,0],[20,1,22,1],[24,0,24,3],[45,4,45,5],[36,0,43,0],[36,1,39,1],[40,1,43,1],[82,4,82,5],[84,0,95,0],[64,0,64,3],[64,4,64,5],[66,0,79,0],[111,0,111,1],[112,0,112,1],[100,0,107,0],[110,0,110,1],[82,0,82,3],[98,0,98,3]]}
[]
["IMPORTES MAXIMOS DE CORTE Y RECONEXION (NO INCLUYE IGV)"]
["Conexiones monofásicas, hasta 10 kW, BT5A, BT5B y BT6"]
[null,null,"Vigente a partir del 04-02-2022"]
["Descripción",null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Fusible o interruptor (tapa sin ranura)",7.2]
[null,null,"Interruptor (tapa con ranura)",9.77]
[null,null,"Caja de medición (aislamiento acometida)",10.48]
[null,null,"Línea aérea (empalme)",25.07]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)",8.69]
[null,null,"Interruptor (tapa con ranura)",11.23]
[null,null,"Caja de medición (aislamiento acometida)",12.04]
[null,null,"Línea aérea (empalme)",30.46]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Retiro","RT conexión aérea","Camioneta",50.37,54.01]
[null,null,"RT conexión subterránea","Camioneta",51.3,54.74]
[null,null,"RT conexión mixta","Camioneta",51.3,54.74]
[null,"Reinstalación","RIconexión aérea","Camioneta",89.03,95.9]
[null,null,"RI conexión subterránea","Camioneta",66.87,72.3]
[null,null,"RI conexión mixta","Camioneta",66.87,72.3]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Monofásica hasta 10 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Caja de medición (aislamiento acometida bloqueada)","Camioneta",23.14,27.03]
[null,"Reconexión","Caja de medición (aislamiento acometida bloqueada)","Camioneta",20.89,25.67]
[null,"Retiro","RT conexión subterránea (empalme y cable de acometida)","Camioneta",171.78,178.65]
[null,null,"RT conexión mixta (empalme y cable de acometida)","Camioneta",171.78,178.65]
[null,"Reinstalación","RI conexión subterránea (empalme y cable de acometida)","Camioneta",237,246.17]
[null,null,"RI conexión mixta (empalme y cable de acometida)","Camioneta",237,246.17]
[]
["Conexiones Trifásicas, hasta 20 kW, BT5A, BT5B y BT6"]
["Descripción",null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Fusible o interruptor (tapa sin ranura)",8.56]
[null,null,"Interruptor (tapa con ranura)",10.88]
[null,null,"Caja de medición (aislamiento acometida)",10.99]
[null,null,"Línea aérea (empalme)",24.82]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)",11.5]
[null,null,"Interruptor (tapa con ranura)",13.41]
[null,null,"Caja de medición (aislamiento acometida)",14.36]
[null,null,"Línea aérea (empalme)",31.32]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Retiro","RT conexión aérea","Camioneta",59.91,64.5]
[null,null,"RT conexión subterránea","Camioneta",55.67,59.1]
[null,null,"RT conexión mixta","Camioneta",55.67,59.1]
[null,"Reinstalación","RI conexión aérea","Camioneta",102.74,110.58]
[null,null,"RI conexión subterránea","Camioneta",75.010000000000005,81.11]
[null,null,"RI conexión mixta","Camioneta",75.010000000000005,81.11]
[]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW BT5A-BT5B-BT5C-AP-BT6","Corte","Caja de medición (aislamiento acometida bloqueada)","Camioneta",26.25,30.83]
[null,"Reconexión","Caja de medición (aislamiento acometida bloqueada)","Camioneta",28.27,31.84]
[null,"Retiro","RT conexión subterránea (empalme y cable de acometida)","Camioneta",188.51,195.38]
[null,null,"RT conexión mixta (empalme y cable de acometida)","Camioneta",188.51,195.38]
[null,"Reinstalación","RI conexión subterránea (empalme y cable de acometida)","Camioneta",276.77,276.77]
[null,null,"RI conexión mixta (empalme y cable de acometida)","Camioneta",267.64,275.68]
[]
["Conexiones Trifásicas, hasta 20 kW, resto de opciones (BT2,BT3 y BT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 20 kW resto de opciones (BT2,BT3 y BT4)","Corte","Fusible o interruptor (tapa sin ranura)","Camioneta",24.19,26.13]
[null,null,"Interruptor (tapa con ranura)","Camioneta",27.06,29.28]
[null,null,"Caja de medición (aislamiento acometida)","Camioneta",27.22,29.39]
[null,null,"Línea aérea (empalme)","Camioneta",38.75,41.51]
[null,"Reconexión","Fusible o interruptor (tapa sin ranura)","Camioneta",39.299999999999997,41.43]
[null,null,"Interruptor (tapa con ranura)","Camioneta",30.6,33.119999999999997]
[null,null,"Caja de medición (aislamiento acometida)","Camioneta",42.94,44.88]
[null,null,"Línea aérea (empalme)","Camioneta",58.17,61.04]
[null,"Retiro","RT conexión aérea","Camioneta",59.91,64.5]
[null,null,"RT conexión subterránea","Camioneta",55.67,59.1]
[null,null,"RT conexión mixta","Camioneta",55.67,59.1]
[null,"Reinstalación","RIconexión aérea","Camioneta",114.46,122.31]
[null,null,"RIión subterránea","Camioneta",86.75,92.88]
[null,null,"RI conexión mixta","Camioneta",86.75,92.88]
[]
["Conexiones trifásicas mayor a 20 kW, resto de opciones (BT2,BT3 y BT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica mayor a 20 kW resto de opciones (BT2,BT3 y BT4)","Corte","En fusible o interruptor (tapa sin ranura)","Camioneta",26.98,29.16]
[null,null,"En caja de medición (aislamiento acometida)","Camioneta",29.51,31.88]
[null,null,"En línea aérea (empalme)","Camioneta",43.84,46.79]
[null,"Reconexión","En fusible o interruptor (tapa sin ranura)","Camioneta",35.369999999999997,37.54]
[null,null,"En caja de medición (aislamiento acometida)","Camioneta",44.26,47.14]
[null,null,"En línea aérea (empalme)","Camioneta",70.86,74.78]
[null,"Retiro","En conexión aérea","Camioneta",87.37,94.19]
[null,null,"En conexión subterránea","Camioneta",81.819999999999993,87.91]
[null,null,"En conexión mixta","Camioneta",81.819999999999993,87.91]
[null,"Reinstalación","En conexión aérea","Camioneta",130.65,139.78]
[null,null,"En conexión subterránea","Camioneta",105.34,113.19]
[null,null,"En conexión mixta","Camioneta",105.34,113.19]
[]
["Conexiones trifásicas, hasta 2500 kW, resto de opciones (MT2,MT3 y MT4)"]
["Descripción",null,null,null,"Costo Total (S/.)"]
["Tipo de Conexión","Tipo","Modalidad","Traslado","Urbana Provincia","Rural"]
["Trifásica hasta 2500 kW resto de opciones (MT2,MT3 y MT4)","Corte","En sistema de protección - PMI","Camioneta",54.98,59.56]
[null,null,"En sistema de protección - Celda","Camioneta",54.94,59.49]
[null,"Reconexión","En sistema de protección - PMI","Camioneta",54.94,59.49]
[null,null,"En sistema de protección - Celda","Camioneta",65.94,71.37]
[null,"Retiro","En sistema de protección - PMI","Camioneta",231.76,240.89]
[null,null,"En sistema de protección - Celda","Camioneta",94.12,101.96]
[null,"Reinstalación","En sistema de protección - PMI","Camioneta",410.22,421.2]
[null,null,"En sistema de protección - Celda","Camioneta",241.9,251.07]
[]
["Suministros Rurales con Celdas Fotovoltaicas (Sierra)"]
["Tipo",null,"Costo Total (S/.)"]
["Corte",null,7.86]
["Reconexión",null,9.85]